| Nano100AN Series BSP V3.02.002 The Board Support Package for Nano100AN Series

gpio.c
Go to the documentation of this file.
1 /**************************************************************************/
12 #include "Nano100Series.h"
13
14
15
40 void GPIO_SetMode(GPIO_T *gpio, uint32_t u32PinMask, uint32_t u32Mode)
41 {
42 uint32_t i;
43
44 for (i=0; i<GPIO_PIN_MAX; i++)
45 {
46 if (u32PinMask & (1 << i))
47 {
48 gpio->PMD = (gpio->PMD & ~(0x3 << (i << 1))) | (u32Mode << (i << 1));
49 }
50 }
51 }
52
65 void GPIO_EnableInt(GPIO_T *gpio, uint32_t u32Pin, uint32_t u32IntAttribs)
66 {
67 gpio->IMD |= (((u32IntAttribs >> 24) & 0xFFUL) << u32Pin);
68 gpio->IER |= ((u32IntAttribs & 0xFFFFFFUL) << u32Pin);
69 }
70
71
82 void GPIO_DisableInt(GPIO_T *gpio, uint32_t u32Pin)
83 {
84 gpio->IMD &= ~(1UL << u32Pin);
85 gpio->IER &= ~((0x00010001UL) << u32Pin);
86 }
87
88
89 /* end of group NANO100_GPIO_EXPORTED_FUNCTIONS */
91 /* end of group NANO100_GPIO_Driver */
93 /* end of group NANO100_Device_Driver */
95
96 /*** (C) COPYRIGHT 2013 Nuvoton Technology Corp. ***/
GPIO_T
Definition: Nano100Series.h:3754
GPIO_DisableInt
void GPIO_DisableInt(GPIO_T *gpio, uint32_t u32Pin)
Disable GPIO interrupt.
Definition: gpio.c:82
Nano100Series.h
Nano100 series peripheral access layer header file. This file contains all the peripheral register's ...
GPIO_T::IMD
__IO uint32_t IMD
Definition: Nano100Series.h:3980
GPIO_T::PMD
__IO uint32_t PMD
Definition: Nano100Series.h:3878
GPIO_EnableInt
void GPIO_EnableInt(GPIO_T *gpio, uint32_t u32Pin, uint32_t u32IntAttribs)
Enable GPIO interrupt.
Definition: gpio.c:65
GPIO_T::IER
__IO uint32_t IER
Definition: Nano100Series.h:4278
GPIO_SetMode
void GPIO_SetMode(GPIO_T *gpio, uint32_t u32PinMask, uint32_t u32Mode)
Set GPIO operation mode.
Definition: gpio.c:40
GPIO_PIN_MAX
#define GPIO_PIN_MAX
Definition: gpio.h:32