| Nano100AN Series BSP V3.02.002 The Board Support Package for Nano100AN Series

Data Fields
COMMAND Struct Reference
NANO100 Library » SDCARD Library » SDCARD Library Exported Structs

`#include <SDCard.h>`

## Data Fields
uint8_t | command_byte
uint8_t | arg_required
uint8_t | CRC
uint8_t | trans_type
uint8_t | response
uint8_t | var_length

## Detailed Description

Definition at line 132 of file SDCard.h.

## Field Documentation

## ◆ arg_required

uint8_t COMMAND::arg_required

Indicates argument requirement;

Definition at line 135 of file SDCard.h.

## ◆ command_byte

uint8_t COMMAND::command_byte

OpCode;

Definition at line 134 of file SDCard.h.

## ◆ CRC

uint8_t COMMAND::CRC

Holds CRC for command if necessary;

Definition at line 136 of file SDCard.h.

## ◆ response

uint8_t COMMAND::response

Indicates expected response;

Definition at line 138 of file SDCard.h.

## ◆ trans_type

uint8_t COMMAND::trans_type

Indicates command transfer type;

Definition at line 137 of file SDCard.h.

## ◆ var_length

uint8_t COMMAND::var_length

Indicates varialble length transfer;

Definition at line 139 of file SDCard.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nano100absp/Library/SDCardLib/SDCard.h