| Airoha M0 BLE API 1.0.5.4

Data Fields
GATT_4_6_2_PARA Struct Reference
ble_gatt_client.h

GATT Client API parameter for ble_gatt_4_6_2_disc_chars_by_UUID. More...

## Data Fields
uint16_t | conn_handle
| connection handle of designated gatt server
uint16_t | start
| first attribute handle of discovering range
uint16_t | end
| last attribute handle of discovering range
uint8_t | uuid_size
| size of uuid
uint8_t | uuid [16]
| uuid in little-endian format

## Detailed Description

GATT Client API parameter for ble_gatt_4_6_2_disc_chars_by_UUID.