| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Macros | Functions
NuEdu-Basic01_LED.c File Reference
`#include <stdio.h>`
`#include "Nano100Series.h"`
`#include "NuEdu-Basic01_LED.h"`

Go to the source code of this file.

## Macros
#define | LED1_ON PB0=0
#define | LED2_ON PB1=0
#define | LED3_ON PE9=0
#define | LED4_ON PE10=0
#define | LED5_ON PE11=0
#define | LED6_ON PD8=0
#define | LED7_ON PD9=0
#define | LED8_ON PC7=0
#define | LED1_OFF PB0=1
#define | LED2_OFF PB1=1
#define | LED3_OFF PE9=1
#define | LED4_OFF PE10=1
#define | LED5_OFF PE11=1
#define | LED6_OFF PD8=1
#define | LED7_OFF PD9=1
#define | LED8_OFF PC7=1

## Functions
void | initial_led (void)
| Set LED GPIO to output mode. More...
void | LED_on (unsigned int temp)
| This function turn on LED numbers to open or close. More...
void | initial_close (void)
| Set LED GPIO to input mode. More...