| Airoha M0 BLE API 1.0.5.4

Data Structures | Functions | Variables
service_trspx.h

## Data Structures
struct | trspx_init_para
| trspx service initialization Parameters More...

## Functions
void | TRSPX_service_init_para (trspx_init_para *para)
| Initialization function of trspx service. More...

## Variables
uint8_t * | trspx_init_para::write_data
uint8_t * | trspx_init_para::read_data
uint8_t * | trspx_init_para::trspx_cccd
ATTCB | trspx_init_para::trspx_write_CB
ATTCB | trspx_init_para::trspx_cccd_CB

## Detailed Description

### service_trspx.h

service_trspx.h provides an easy way to implement TRSPX service.

## Function Documentation

## ◆ TRSPX_service_init_para()

void TRSPX_service_init_para | ( | trspx_init_para * | para | ) |

Initialization function of trspx service.

Parameters

  para | trspx_init_para.

Returns
  None.

## Variable Documentation

## ◆ write_data

uint8_t* trspx_init_para::write_data

Data buffer pointer for receiving data

## ◆ read_data

uint8_t* trspx_init_para::read_data

Data buffer pointer for sending data

## ◆ trspx_cccd

uint8_t* trspx_init_para::trspx_cccd

Data buffer pointer for cccd

## ◆ trspx_write_CB

ATTCB trspx_init_para::trspx_write_CB

callback function for GATT write operation

## ◆ trspx_cccd_CB

ATTCB trspx_init_para::trspx_cccd_CB

callback function for CCCD descriptor write