| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Macros
PWM Exported Constants
NANO100 Device Driver » PWM Driver

## Macros
#define | PWM_CHANNEL_NUM
#define | PWM_CH0
#define | PWM_CH1
#define | PWM_CH2
#define | PWM_CH3
#define | PWM_CH_0_MASK
#define | PWM_CH_1_MASK
#define | PWM_CH_2_MASK
#define | PWM_CH_3_MASK
#define | PWM_CLK_DIV_1
#define | PWM_CLK_DIV_2
#define | PWM_CLK_DIV_4
#define | PWM_CLK_DIV_8
#define | PWM_CLK_DIV_16
#define | PWM_EDGE_ALIGNED
#define | PWM_CENTER_ALIGNED
#define | PWM_RISING_LATCH_INT_ENABLE
#define | PWM_FALLING_LATCH_INT_ENABLE
#define | PWM_RISING_FALLING_LATCH_INT_ENABLE
#define | PWM_RISING_LATCH_INT_FLAG
#define | PWM_FALLING_LATCH_INT_FLAG
#define | PWM_RISING_FALLING_LATCH_INT_FLAG
#define | PWM_RISING_LATCH_PDMA_ENABLE
#define | PWM_FALLING_LATCH_PDMA_ENABLE
#define | PWM_RISING_FALLING_LATCH_PDMA_ENABLE
#define | PWM_CAP_PDMA_RFORDER_R
#define | PWM_CAP_PDMA_RFORDER_F

## Detailed Description

## Macro Definition Documentation

## ◆ PWM_CAP_PDMA_RFORDER_F

#define PWM_CAP_PDMA_RFORDER_F

PWM captured data transferred by PDMA is falling latch first

Definition at line 58 of file pwm.h.

## ◆ PWM_CAP_PDMA_RFORDER_R

#define PWM_CAP_PDMA_RFORDER_R

PWM captured data transferred by PDMA is rising latch first

Definition at line 57 of file pwm.h.

## ◆ PWM_CENTER_ALIGNED

#define PWM_CENTER_ALIGNED

PWM working in center aligned type

Definition at line 47 of file pwm.h.

## ◆ PWM_CH0

#define PWM_CH0

PWM channel 0

Definition at line 33 of file pwm.h.

## ◆ PWM_CH1

#define PWM_CH1

PWM channel 1

Definition at line 34 of file pwm.h.

## ◆ PWM_CH2

#define PWM_CH2

PWM channel 2

Definition at line 35 of file pwm.h.

## ◆ PWM_CH3

#define PWM_CH3

PWM channel 3

Definition at line 36 of file pwm.h.

## ◆ PWM_CH_0_MASK

#define PWM_CH_0_MASK

PWM channel 0 mask

Definition at line 37 of file pwm.h.

## ◆ PWM_CH_1_MASK

#define PWM_CH_1_MASK

PWM channel 1 mask

Definition at line 38 of file pwm.h.

## ◆ PWM_CH_2_MASK

#define PWM_CH_2_MASK

PWM channel 2 mask

Definition at line 39 of file pwm.h.

## ◆ PWM_CH_3_MASK

#define PWM_CH_3_MASK

PWM channel 3 mask

Definition at line 40 of file pwm.h.

## ◆ PWM_CHANNEL_NUM

#define PWM_CHANNEL_NUM

PWM channel number

Definition at line 32 of file pwm.h.

## ◆ PWM_CLK_DIV_1

#define PWM_CLK_DIV_1

PWM clock divide by 1

Definition at line 41 of file pwm.h.

## ◆ PWM_CLK_DIV_16

#define PWM_CLK_DIV_16

PWM clock divide by 16

Definition at line 45 of file pwm.h.

## ◆ PWM_CLK_DIV_2

#define PWM_CLK_DIV_2

PWM clock divide by 2

Definition at line 42 of file pwm.h.

## ◆ PWM_CLK_DIV_4

#define PWM_CLK_DIV_4

PWM clock divide by 4

Definition at line 43 of file pwm.h.

## ◆ PWM_CLK_DIV_8

#define PWM_CLK_DIV_8

PWM clock divide by 8

Definition at line 44 of file pwm.h.

## ◆ PWM_EDGE_ALIGNED

#define PWM_EDGE_ALIGNED

PWM working in edge aligned type

Definition at line 46 of file pwm.h.

## ◆ PWM_FALLING_LATCH_INT_ENABLE

#define PWM_FALLING_LATCH_INT_ENABLE

PWM falling latch interrupt enable

Definition at line 49 of file pwm.h.

## ◆ PWM_FALLING_LATCH_INT_FLAG

#define PWM_FALLING_LATCH_INT_FLAG

PWM falling latch condition happened

Definition at line 52 of file pwm.h.

## ◆ PWM_FALLING_LATCH_PDMA_ENABLE

#define PWM_FALLING_LATCH_PDMA_ENABLE

PWM falling latch PDMA enable

Definition at line 55 of file pwm.h.

## ◆ PWM_RISING_FALLING_LATCH_INT_ENABLE

#define PWM_RISING_FALLING_LATCH_INT_ENABLE

PWM rising latch interrupt enable

Definition at line 50 of file pwm.h.

## ◆ PWM_RISING_FALLING_LATCH_INT_FLAG

#define PWM_RISING_FALLING_LATCH_INT_FLAG

PWM rising latch condition happened

Definition at line 53 of file pwm.h.

## ◆ PWM_RISING_FALLING_LATCH_PDMA_ENABLE

#define PWM_RISING_FALLING_LATCH_PDMA_ENABLE

PWM rising and falling latch PDMA enable

Definition at line 56 of file pwm.h.

## ◆ PWM_RISING_LATCH_INT_ENABLE

#define PWM_RISING_LATCH_INT_ENABLE

PWM rising latch interrupt enable

Definition at line 48 of file pwm.h.

## ◆ PWM_RISING_LATCH_INT_FLAG

#define PWM_RISING_LATCH_INT_FLAG

PWM rising latch condition happened

Definition at line 51 of file pwm.h.

## ◆ PWM_RISING_LATCH_PDMA_ENABLE

#define PWM_RISING_LATCH_PDMA_ENABLE

PWM rising latch PDMA enable

Definition at line 54 of file pwm.h.