| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Data Fields
SCLIB_CARD_INFO_T Struct Reference
NANO100 Library » Smartcard Library » Smartcard Library Exported Structs

A structure holds smartcard information. More...

`#include <sclib.h>`

## Data Fields
uint32_t | T
| Protocol, ether SCLIB_PROTOCOL_T0 or SCLIB_PROTOCOL_T1. More...
uint32_t | ATR_Len
| ATR length, between SCLIB_MAX_ATR_LEN and SCLIB_MIN_ATR_LEN. More...
uint8_t | ATR_Buf [SCLIB_MAX_ATR_LEN]
| Buffer holds ATR answered by smartcard. More...

## Detailed Description

A structure holds smartcard information.

Definition at line 93 of file sclib.h.

## Field Documentation

## ◆ ATR_Buf

uint8_t SCLIB_CARD_INFO_T::ATR_Buf[SCLIB_MAX_ATR_LEN]

Buffer holds ATR answered by smartcard.

Definition at line 97 of file sclib.h.

## ◆ ATR_Len

uint32_t SCLIB_CARD_INFO_T::ATR_Len

ATR length, between SCLIB_MAX_ATR_LEN and SCLIB_MIN_ATR_LEN.

Definition at line 96 of file sclib.h.

## ◆ T

uint32_t SCLIB_CARD_INFO_T::T

Protocol, ether SCLIB_PROTOCOL_T0 or SCLIB_PROTOCOL_T1.

Definition at line 95 of file sclib.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nano100bbsp/Library/SmartcardLib/Include/sclib.h