| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_RGBLED.h File Reference

NuEdu-Basic01 RGB LED driver header file for NuEdu-SDK-Nano130. More...

Go to the source code of this file.

## Functions
void | Initial_PWM_LED (void)
| Set multi-function pins for PWM0 channel 0,1,2. More...
void | PWM_LED (void)
| Set PWM clock enable and HCLK as PWM clock source, PWM frequency is 100Hz, duty 30% and enable output of all PWM channels. More...

## Detailed Description

NuEdu-Basic01 RGB LED driver header file for NuEdu-SDK-Nano130.

Version
  V1.00

Revision
  4

Date
  14/10/17 4:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_RGBLED.h.