| Airoha M0 BLE API 1.0.5.4

Data Fields
GATT_4_9_5_PARA Struct Reference
ble_gatt_client.h

GATT Client API parameter for ble_gatt_4_9_5_reliable_writes. More...

## Data Fields
uint16_t | conn_handle
| connection handle of designated gatt server
uint16_t | att_handle
| attribute handle to be written
uint16_t | len
| length of attribute data (10 bytes at most)
uint16_t | offset
| offset of attribute data
uint8_t | value [10]
| attribute data

## Detailed Description

GATT Client API parameter for ble_gatt_4_9_5_reliable_writes.