| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gatt_evt_mtu_exchange_t Struct Reference
ble_gatt_client.h

Event parameter of gatt event BLE_GATT_EVT_MTU_EXCHANGED. More...

## Data Fields
uint16_t | conn_handle

## Detailed Description

Event parameter of gatt event BLE_GATT_EVT_MTU_EXCHANGED.

## Field Documentation

## ◆ conn_handle

uint16_t ble_gatt_evt_mtu_exchange_t::conn_handle

new mtu size negotiated with gatt server