| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

NuEdu-Basic01_LED.h
Go to the documentation of this file.
1 /****************************************************************************/
12 #ifndef __NuEdu_Basic01_12LED_H__
13 #define __NuEdu_Basic01_12LED_H__
14
26 extern void initial_led(void);
27 extern void LED_on(unsigned int temp); /* end of group Nano130_Basic01_FUNCTIONS */
29 /* end of group NuEdu-SDK-Nano130_Basic01 */
31 /* end of group NANO100_Library */
33
34 #endif
35 /*** (C) COPYRIGHT 2013-2014 Nuvoton Technology Corp. ***/
initial_led
void initial_led(void)
Set LED GPIO to output mode.
Definition: NuEdu-Basic01_LED.c:54
LED_on
void LED_on(unsigned int temp)
This function turn on LED numbers to open or close.
Definition: NuEdu-Basic01_LED.c:75