| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gap_evt_conn_param_update_request_t Struct Reference
ble_gap.h

Event structure for BLE_GAP_EVT_CONN_PARAM_UPDATE_REQUEST. More...

## Data Fields
uint16_t | handle
| connection handler
uint16_t | identifier
| identifier used to reponse
uint16_t | min_conn_interval
| Minimum Connection Interval in 1.25 ms units.
uint16_t | max_conn_interval
| Maximum Connection Interval in 1.25 ms units.
uint16_t | slave_latency
| Slave Latency in number of connection events.
uint16_t | conn_sup_timeout
| Connection Supervision Timeout in 10 ms units.

## Detailed Description

Event structure for BLE_GAP_EVT_CONN_PARAM_UPDATE_REQUEST.