| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

NuEdu-Basic01_PWMDAC.h
Go to the documentation of this file.
1 /****************************************************************************/
13 #ifndef __NuEdu_Basic01_PWMDAC_H__
14 #define __NuEdu_Basic01_PWMDAC_H__
15
16
29 extern void Initial_PWM_DAC(void);
30 extern void Write_PWMDAC(void); /* end of group Nano130_Basic01_FUNCTIONS */
32 /* end of group NuEdu-SDK-Nano130_Basic01 */
34 /* end of group NANO100_Library */
36 #endif
37
38 /*** (C) COPYRIGHT 2013-2014 Nuvoton Technology Corp. ***/
Write_PWMDAC
void Write_PWMDAC(void)
This function is used to set PWM for PWM DAC.
Definition: NuEdu-Basic01_PWMDAC.c:33
Initial_PWM_DAC
void Initial_PWM_DAC(void)
This function is used to setup multi-function pin of PC12 for PWM1_CH0.
Definition: NuEdu-Basic01_PWMDAC.c:51