| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_LED.h File Reference

Nano100 series Basic01 board LED driver header file. More...

Go to the source code of this file.

## Functions
void | initial_led (void)
| Set LED GPIO to output mode. More...
void | LED_on (unsigned int temp)
| This function turn on LED numbers to open or close. More...

## Detailed Description

Nano100 series Basic01 board LED driver header file.

Version
  V1.00

Revision
  4

Date
  14/10/17 4:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_LED.h.