| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_SPI_Flash.h File Reference

NuEdu-Basic01 SPI Flash driver header file for NuEdu-SDK-Nano130. More...

Go to the source code of this file.

## Functions
void | Open_SPI_Flash (void)
| Open GPIO port for SPI interface and configure this SPI controller as Master, MSB first, clock idle low, TX at falling-edge, RX at rising-edge, 32-bit length transaction, disable the automatic hardware slave select function and SPI serial clock rate = 2 MHz. More...
unsigned int | SpiFlash_ReadMidDid (void)
| Read back the Manufacturer ID and Device ID from SPI Flash device. More...
void | SpiFlash_ChipErase (void)
| This function do the chip erasing to SPI Flash device. More...
unsigned int | SpiFlash_ReadStatusReg1 (void)
| Read back the Status Register 1 from SPI Flash device. More...
unsigned int | SpiFlash_ReadStatusReg2 (void)
| Read back the Status Register 2 from SPI Flash device. More...
void | SpiFlash_WaitReady (void)
| Waiting for the BUSY bit of SPI Flash that be cleared to 0. More...
void | SpiFlash_PageProgram (unsigned char *DataBuffer, unsigned int StartAddress, unsigned int ByteCount)
| This function do the page programming to SPI Flash device. More...
void | SpiFlash_ReadData (unsigned char *DataBuffer, unsigned int StartAddress, unsigned int ByteCount)
| This function do the data reading from SPI Flash device. More...

## Detailed Description

NuEdu-Basic01 SPI Flash driver header file for NuEdu-SDK-Nano130.

Version
  V1.00

Revision
  4

Date
  14/10/17 4:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_SPI_Flash.h.