| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gap_evt_conn_param_update_t Struct Reference
ble_gap.h

Event structure for BLE_GAP_EVT_CONNECT_PARM_UPDATE. More...

## Data Fields
uint8_t | status
| 0: success else fail
uint16_t | conn_handle
| Connection Handle.
uint16_t | conn_interval
| Connection Interval in 1.25 ms units,.
uint16_t | slave_latency
| Slave Latency in number of connection events.
uint16_t | conn_sup_timeout
| Connection Supervision Timeout in 10 ms units.

## Detailed Description

Event structure for BLE_GAP_EVT_CONNECT_PARM_UPDATE.