| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gatt_evt_multi_char_read_t Struct Reference
ble_gatt_client.h

Event parameter of gatt event BLE_GATT_EVT_MULTI_CHAR_READ. More...

## Data Fields
uint16_t | handle [5]
uint16_t | len
uint8_t | value [1]

## Detailed Description

Event parameter of gatt event BLE_GATT_EVT_MULTI_CHAR_READ.

## Field Documentation

## ◆ handle

uint16_t ble_gatt_evt_multi_char_read_t::handle[5]

number of characteristics read in this event

## ◆ len

uint16_t ble_gatt_evt_multi_char_read_t::len

array of characteristic handle

## ◆ value

uint8_t ble_gatt_evt_multi_char_read_t::value[1]

length of packed characteristic values