| Airoha M0 BLE API 1.0.5.4

Data Fields
hids_char_report_map_t Struct Reference
service_human_interface_device.h

Report map characteristic initialization parameters. More...

## Data Fields
uint8_t * | data
uint16_t | data_len
uint16_t | ext_rep_ref_uuid [MAX_EXT_REP_REF_NUM]
uint16_t | included_service_handle [MAX_INCLUDED_SERVICE_NUM]
uint8_t | ext_rep_ref_uuid_num
uint8_t | included_service_num

## Detailed Description

Report map characteristic initialization parameters.

## Field Documentation

## ◆ data

uint8_t* hids_char_report_map_t::data

hid report map data pointer

## ◆ data_len

uint16_t hids_char_report_map_t::data_len

hid report map data length

## ◆ ext_rep_ref_uuid

uint16_t hids_char_report_map_t::ext_rep_ref_uuid[MAX_EXT_REP_REF_NUM]

list of extended report reference UUID

## ◆ included_service_handle

uint16_t hids_char_report_map_t::included_service_handle[MAX_INCLUDED_SERVICE_NUM]

list of included service attribute handle

## ◆ ext_rep_ref_uuid_num

uint8_t hids_char_report_map_t::ext_rep_ref_uuid_num

number of extended report reference UUIDs, must< MAX_EXT_REP_REF_NUM

## ◆ included_service_num

uint8_t hids_char_report_map_t::included_service_num

number of included services, must <MAX_INCLUDED_SERVICE_NUM