| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gatt_evt_reliable_write_finished_t Struct Reference
ble_gatt_client.h

Event parameter of gatt event BLE_GATT_EVT_RELIABLE_WRITE_FINISHED. More...

## Data Fields
uint8_t | num

## Detailed Description

Event parameter of gatt event BLE_GATT_EVT_RELIABLE_WRITE_FINISHED.

## Field Documentation

## ◆ num

uint8_t ble_gatt_evt_reliable_write_finished_t::num

0: data was written successfully.
1: write procedure was canceled since returned data is different from original request