| Airoha M0 BLE API 1.0.5.4

Data Fields
GATT_4_3_1_PARA Struct Reference
ble_gatt_client.h

GATT Client API parameter for ble_gatt_4_3_1_exchange_mtu. More...

## Data Fields
uint16_t | conn_handle
| connection handle of designated gatt server
uint16_t | mtu
| desired mtu size to be negotiated (only 23~200 is supported)

## Detailed Description

GATT Client API parameter for ble_gatt_4_3_1_exchange_mtu.