| Airoha M0 BLE API 1.0.5.4

Data Fields
hids_char_hid_control_point_t Struct Reference
service_human_interface_device.h

HID control point characteristic initialization parameters. More...

## Data Fields
uint8_t * | data
ATTCB | cb

## Detailed Description

HID control point characteristic initialization parameters.

## Field Documentation

## ◆ data

uint8_t* hids_char_hid_control_point_t::data

hid control point data pointer

## ◆ cb

ATTCB hids_char_hid_control_point_t::cb

hid control pointer call bacck function