| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gap_conn_params_t Struct Reference
ble_gap.h

parameters for a link It is usually used for updating parameters of a connection. More...

## Data Fields
uint16_t | min_conn_interval
| Minimum Connection Interval in 1.25 ms units.
uint16_t | max_conn_interval
| Maximum Connection Interval in 1.25 ms units.
uint16_t | slave_latency
| Slave Latency in number of connection events.
uint16_t | conn_sup_timeout
| Connection Supervision Timeout in 10 ms units.
uint16_t | ce_min
| Minimal CE.
uint16_t | ce_max
| Maximal CE.

## Detailed Description

parameters for a link It is usually used for updating parameters of a connection.