| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

NuEdu-Basic01_System.h
Go to the documentation of this file.
1 /**************************************************************************/
12 #ifndef __NuEdu_Basic01_System_H__
13 #define __NuEdu_Basic01_System_H__
14
15 #ifdef __cplusplus
16 extern "C"
17 {
18 #endif
19
32 void SYS_Init(void);
33
34 /* end of group Nano130_Basic01_FUNCTIONS System Exported Functions */
36 /* end of group NuEdu-SDK-Nano130_Basic01 Nano130_Basic01 Library */
38 /* end of group NANO100_Library NANO100 Library */
40
41 #ifdef __cplusplus
42 }
43 #endif
44
45 #endif //__NuEdu_Basic01_System_H__
46 /*** (C) COPYRIGHT 2013-2014 Nuvoton Technology Corp. ***/
SYS_Init
void SYS_Init(void)
This function enables HXT, LXT and LIRC clock and sets HCLK source from HXT to 42MHz.
Definition: NuEdu-Basic01_System.c:37