| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions | Variables
NuEdu-Basic01_PWM_Capture.c File Reference

NuEdu-Basic01_PWM_Capture driver source file for NuEdu-SDK-Nano130. More...

`#include <stdio.h>`
`#include "NUC200Series.h"`
`#include "NuEdu-Basic01_PWM_Capture.h"`

Go to the source code of this file.

## Functions
void | Open_PWM6_OUT (uint32_t PWM_Frequency, uint32_t PWM_Duty)
void | Close_PWM6_OUT (void)
void | Open_PWM7_Capture (void)
void | Close_PWM7_Capture (void)
void | Get_PWM7_Capture_Data (void)
void | Open_PWM3_Capture (void)
void | Close_PWM3_Capture (void)
void | Get_PWM3_Capture_Data (void)

## Variables
uint32_t | PWM23_Clock = 1000000
uint32_t | PWM67_Clock = 1000000
uint32_t | Open_PWM6_OUT_Fail = FALSE
uint32_t | Open_PWM3_Capture_Fail = FALSE
uint32_t | Open_PWM7_Capture_Fail = FALSE
PWM_Capture_T | PWM3 = {0,0,0,0,0,0,0}
PWM_Capture_T | PWM7 = {0,0,0,0,0,0,0}

## Detailed Description

NuEdu-Basic01_PWM_Capture driver source file for NuEdu-SDK-Nano130.

Version
  V1.00

Revision
  3

Date
  14/09/12 11:15p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_PWM_Capture.c.

## Variable Documentation

## ◆ PWM23_Clock

uint32_t PWM23_Clock = 1000000

Definition at line 16 of file NuEdu-Basic01_PWM_Capture.c.