| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Data Fields
PWM_Capture_T Struct Reference
NANO100 Library » Nano130_Basic01 Library » Basic01 peripheral Functions

`#include <NuEdu-Basic01_PWM_Capture.h>`

## Data Fields
__IO uint32_t | Capture_Rising [2]
__IO uint32_t | Capture_Falling [2]
__IO uint32_t | Last_Edge
__IO uint32_t | High_Period
__IO uint32_t | Low_Period
__IO uint32_t | Signal_Period
__IO float | Signal_Frequency

## Detailed Description

Definition at line 30 of file NuEdu-Basic01_PWM_Capture.h.

## Field Documentation

## ◆ Capture_Falling

__IO uint32_t PWM_Capture_T::Capture_Falling[2]

Definition at line 33 of file NuEdu-Basic01_PWM_Capture.h.

## ◆ Capture_Rising

__IO uint32_t PWM_Capture_T::Capture_Rising[2]

Definition at line 32 of file NuEdu-Basic01_PWM_Capture.h.

## ◆ High_Period

__IO uint32_t PWM_Capture_T::High_Period

Definition at line 35 of file NuEdu-Basic01_PWM_Capture.h.

## ◆ Last_Edge

__IO uint32_t PWM_Capture_T::Last_Edge

Definition at line 34 of file NuEdu-Basic01_PWM_Capture.h.

## ◆ Low_Period

__IO uint32_t PWM_Capture_T::Low_Period

Definition at line 36 of file NuEdu-Basic01_PWM_Capture.h.

## ◆ Signal_Frequency

__IO float PWM_Capture_T::Signal_Frequency

Definition at line 38 of file NuEdu-Basic01_PWM_Capture.h.

## ◆ Signal_Period

__IO uint32_t PWM_Capture_T::Signal_Period

Definition at line 37 of file NuEdu-Basic01_PWM_Capture.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nano100bbsp/Library/NuEdu/inc/NuEdu-Basic01_PWM_Capture.h