| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_System.h File Reference

NuEdu-Basic01 System driver header file. More...

Go to the source code of this file.

## Functions
void | SYS_Init (void)
| This function enables HXT, LXT and LIRC clock and sets HCLK source from HXT to 42MHz. More...

## Detailed Description

NuEdu-Basic01 System driver header file.

NuEdu-Basic01 Volume_Knob driver header file.

Version
  V1.00

Revision
  3

Date
  14/10/17 4:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Version
  V1.00

Revision
  2

Date
  14/10/17 4:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Version
  V1.00

Revision
  3

Date
  14/10/17 4:45p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_System.h.