| Airoha M0 BLE API 1.0.5.4

Data Fields
hids_char_hid_information_t Struct Reference
service_human_interface_device.h

HID information characteristic initialization parameters. More...

## Data Fields
uint16_t | bcdHID
uint8_t | bCountryCode
uint8_t | flags

## Detailed Description

HID information characteristic initialization parameters.

## Field Documentation

## ◆ bcdHID

uint16_t hids_char_hid_information_t::bcdHID

version number of base USB HID Spec.

## ◆ bCountryCode

uint8_t hids_char_hid_information_t::bCountryCode

Identifies which country the hardware is localized for.

## ◆ flags

uint8_t hids_char_hid_information_t::flags

Bit mask
Bit0: RemoteWake.
Bit1: NormallyConnectable.