| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

### - u -

- UART0 : Nano100Series.h
- UART0_BASE : Nano100Series.h
- UART0_MODULE : clk.h
- UART0_RST : sys.h
- UART1 : Nano100Series.h
- UART1_BASE : Nano100Series.h
- UART1_MODULE : clk.h
- UART1_RST : sys.h
- UART_ALT_CTL_ADDR_PID_MATCH_Msk : Nano100Series.h
- UART_ALT_CTL_ADDR_PID_MATCH_Pos : Nano100Series.h
- UART_ALT_CTL_Bit_ERR_EN_Msk : Nano100Series.h
- UART_ALT_CTL_Bit_ERR_EN_Pos : Nano100Series.h
- UART_ALT_CTL_LIN_HEAD_SEL_Msk : Nano100Series.h
- UART_ALT_CTL_LIN_HEAD_SEL_Pos : Nano100Series.h
- UART_ALT_CTL_LIN_RX_EN_Msk : Nano100Series.h
- UART_ALT_CTL_LIN_RX_EN_Pos : Nano100Series.h
- UART_ALT_CTL_LIN_TX_BCNT_Msk : Nano100Series.h
- UART_ALT_CTL_LIN_TX_BCNT_Pos : Nano100Series.h
- UART_ALT_CTL_LIN_TX_EN_Msk : Nano100Series.h
- UART_ALT_CTL_LIN_TX_EN_Pos : Nano100Series.h
- UART_ALT_CTL_RS485_AAD_Msk : Nano100Series.h
- UART_ALT_CTL_RS485_AAD_Pos : Nano100Series.h
- UART_ALT_CTL_RS485_ADD_EN_Msk : Nano100Series.h
- UART_ALT_CTL_RS485_ADD_EN_Pos : Nano100Series.h
- UART_ALT_CTL_RS485_AUD_Msk : Nano100Series.h
- UART_ALT_CTL_RS485_AUD_Pos : Nano100Series.h
- UART_ALT_CTL_RS485_NMM_Msk : Nano100Series.h
- UART_ALT_CTL_RS485_NMM_Pos : Nano100Series.h
- UART_BAUD_BRD_Msk : Nano100Series.h
- UART_BAUD_BRD_Pos : Nano100Series.h
- UART_BAUD_DIV_16_EN_Msk : Nano100Series.h
- UART_BAUD_DIV_16_EN_Pos : Nano100Series.h
- UART_BAUD_MODE0 : uart.h
- UART_BAUD_MODE0_DIVIDER : uart.h
- UART_BAUD_MODE1 : uart.h
- UART_BAUD_MODE1_DIVIDER : uart.h
- UART_CTL_ABAUD_EN_Msk : Nano100Series.h
- UART_CTL_ABAUD_EN_Pos : Nano100Series.h
- UART_CTL_AUTO_CTS_EN_Msk : Nano100Series.h
- UART_CTL_AUTO_CTS_EN_Pos : Nano100Series.h
- UART_CTL_AUTO_RTS_EN_Msk : Nano100Series.h
- UART_CTL_AUTO_RTS_EN_Pos : Nano100Series.h
- UART_CTL_DMA_RX_EN_Msk : Nano100Series.h
- UART_CTL_DMA_RX_EN_Pos : Nano100Series.h
- UART_CTL_DMA_TX_EN_Msk : Nano100Series.h
- UART_CTL_DMA_TX_EN_Pos : Nano100Series.h
- UART_CTL_RX_DIS_Msk : Nano100Series.h
- UART_CTL_RX_DIS_Pos : Nano100Series.h
- UART_CTL_RX_RST_Msk : Nano100Series.h
- UART_CTL_RX_RST_Pos : Nano100Series.h
- UART_CTL_TX_DIS_Msk : Nano100Series.h
- UART_CTL_TX_DIS_Pos : Nano100Series.h
- UART_CTL_TX_RST_Msk : Nano100Series.h
- UART_CTL_TX_RST_Pos : Nano100Series.h
- UART_CTL_WAKE_CTS_EN_Msk : Nano100Series.h
- UART_CTL_WAKE_CTS_EN_Pos : Nano100Series.h
- UART_CTL_WAKE_DATA_EN_Msk : Nano100Series.h
- UART_CTL_WAKE_DATA_EN_Pos : Nano100Series.h
- UART_DAT_DAT_Msk : Nano100Series.h
- UART_DAT_DAT_Pos : Nano100Series.h
- UART_DISABLE_INT : uart.h
- UART_ENABLE_INT : uart.h
- UART_FSR_BI_F_Msk : Nano100Series.h
- UART_FSR_BI_F_Pos : Nano100Series.h
- UART_FSR_FE_F_Msk : Nano100Series.h
- UART_FSR_FE_F_Pos : Nano100Series.h
- UART_FSR_PE_F_Msk : Nano100Series.h
- UART_FSR_PE_F_Pos : Nano100Series.h
- UART_FSR_RX_EMPTY_F_Msk : Nano100Series.h
- UART_FSR_RX_EMPTY_F_Pos : Nano100Series.h
- UART_FSR_RX_FULL_F_Msk : Nano100Series.h
- UART_FSR_RX_FULL_F_Pos : Nano100Series.h
- UART_FSR_RX_OVER_F_Msk : Nano100Series.h
- UART_FSR_RX_OVER_F_Pos : Nano100Series.h
- UART_FSR_RX_POINTER_F_Msk : Nano100Series.h
- UART_FSR_RX_POINTER_F_Pos : Nano100Series.h
- UART_FSR_TE_F_Msk : Nano100Series.h
- UART_FSR_TE_F_Pos : Nano100Series.h
- UART_FSR_TX_EMPTY_F_Msk : Nano100Series.h
- UART_FSR_TX_EMPTY_F_Pos : Nano100Series.h
- UART_FSR_TX_FULL_F_Msk : Nano100Series.h
- UART_FSR_TX_FULL_F_Pos : Nano100Series.h
- UART_FSR_TX_OVER_F_Msk : Nano100Series.h
- UART_FSR_TX_OVER_F_Pos : Nano100Series.h
- UART_FSR_TX_POINTER_F_Msk : Nano100Series.h
- UART_FSR_TX_POINTER_F_Pos : Nano100Series.h
- UART_FUN_SEL_FUN_SEL_Msk : Nano100Series.h
- UART_FUN_SEL_FUN_SEL_Pos : Nano100Series.h
- UART_FUNC_SEL_IrDA : uart.h
- UART_FUNC_SEL_LIN : uart.h
- UART_FUNC_SEL_RS485 : uart.h
- UART_FUNC_SEL_UART : uart.h
- UART_GET_INT_FLAG : uart.h
- UART_GET_RX_EMPTY : uart.h
- UART_GET_RX_FULL : uart.h
- UART_GET_TX_EMPTY : uart.h
- UART_GET_TX_FULL : uart.h
- UART_IER_ABAUD_IE_Msk : Nano100Series.h
- UART_IER_ABAUD_IE_Pos : Nano100Series.h
- UART_IER_BUF_ERR_IE_Msk : Nano100Series.h
- UART_IER_BUF_ERR_IE_Pos : Nano100Series.h
- UART_IER_LIN_IE_Msk : Nano100Series.h
- UART_IER_LIN_IE_Pos : Nano100Series.h
- UART_IER_MODEM_IE_Msk : Nano100Series.h
- UART_IER_MODEM_IE_Pos : Nano100Series.h
- UART_IER_RDA_IE_Msk : Nano100Series.h
- UART_IER_RDA_IE_Pos : Nano100Series.h
- UART_IER_RLS_IE_Msk : Nano100Series.h
- UART_IER_RLS_IE_Pos : Nano100Series.h
- UART_IER_RTO_IE_Msk : Nano100Series.h
- UART_IER_RTO_IE_Pos : Nano100Series.h
- UART_IER_THRE_IE_Msk : Nano100Series.h
- UART_IER_THRE_IE_Pos : Nano100Series.h
- UART_IER_WAKE_IE_Msk : Nano100Series.h
- UART_IER_WAKE_IE_Pos : Nano100Series.h
- UART_IRCR_INV_RX_Msk : Nano100Series.h
- UART_IRCR_INV_RX_Pos : Nano100Series.h
- UART_IRCR_INV_TX_Msk : Nano100Series.h
- UART_IRCR_INV_TX_Pos : Nano100Series.h
- UART_IRCR_TX_SELECT_Msk : Nano100Series.h
- UART_IRCR_TX_SELECT_Pos : Nano100Series.h
- UART_IS_RX_FULL : uart.h
- UART_IS_RX_READY : uart.h
- UART_IS_TX_EMPTY : uart.h
- UART_IS_TX_FULL : uart.h
- UART_ISR_ABAUD_IS_Msk : Nano100Series.h
- UART_ISR_ABAUD_IS_Pos : Nano100Series.h
- UART_ISR_BUF_ERR_IS_Msk : Nano100Series.h
- UART_ISR_BUF_ERR_IS_Pos : Nano100Series.h
- UART_ISR_LIN_IS_Msk : Nano100Series.h
- UART_ISR_LIN_IS_Pos : Nano100Series.h
- UART_ISR_MODEM_IS_Msk : Nano100Series.h
- UART_ISR_MODEM_IS_Pos : Nano100Series.h
- UART_ISR_RDA_IS_Msk : Nano100Series.h
- UART_ISR_RDA_IS_Pos : Nano100Series.h
- UART_ISR_RLS_IS_Msk : Nano100Series.h
- UART_ISR_RLS_IS_Pos : Nano100Series.h
- UART_ISR_RTO_IS_Msk : Nano100Series.h
- UART_ISR_RTO_IS_Pos : Nano100Series.h
- UART_ISR_THRE_IS_Msk : Nano100Series.h
- UART_ISR_THRE_IS_Pos : Nano100Series.h
- UART_ISR_WAKE_IS_Msk : Nano100Series.h
- UART_ISR_WAKE_IS_Pos : Nano100Series.h
- UART_MCSR_CTS_ST_Msk : Nano100Series.h
- UART_MCSR_CTS_ST_Pos : Nano100Series.h
- UART_MCSR_DCT_F_Msk : Nano100Series.h
- UART_MCSR_DCT_F_Pos : Nano100Series.h
- UART_MCSR_LEV_CTS_Msk : Nano100Series.h
- UART_MCSR_LEV_CTS_Pos : Nano100Series.h
- UART_MCSR_LEV_RTS_Msk : Nano100Series.h
- UART_MCSR_LEV_RTS_Pos : Nano100Series.h
- UART_MCSR_RTS_ST_Msk : Nano100Series.h
- UART_MCSR_RTS_ST_Pos : Nano100Series.h
- UART_PARITY_EVEN : uart.h
- UART_PARITY_MARK : uart.h
- UART_PARITY_NONE : uart.h
- UART_PARITY_ODD : uart.h
- UART_PARITY_SPACE : uart.h
- UART_READ : uart.h
- UART_RS485_CLEAR_ADDR_FLAG : uart.h
- UART_RS485_GET_ADDR_FLAG : uart.h
- UART_RTS_IS_HIGH_LEV_TRG : uart.h
- UART_RTS_IS_LOW_LEV_TRG : uart.h
- UART_STOP_BIT_1 : uart.h
- UART_STOP_BIT_1_5 : uart.h
- UART_STOP_BIT_2 : uart.h
- UART_TLCTL_BCB_Msk : Nano100Series.h
- UART_TLCTL_BCB_Pos : Nano100Series.h
- UART_TLCTL_DATA_LEN_Msk : Nano100Series.h
- UART_TLCTL_DATA_LEN_Pos : Nano100Series.h
- UART_TLCTL_EPE_Msk : Nano100Series.h
- UART_TLCTL_EPE_Pos : Nano100Series.h
- UART_TLCTL_NSB_Msk : Nano100Series.h
- UART_TLCTL_NSB_Pos : Nano100Series.h
- UART_TLCTL_PBE_Msk : Nano100Series.h
- UART_TLCTL_PBE_Pos : Nano100Series.h
- UART_TLCTL_RFITL_14BYTES : uart.h
- UART_TLCTL_RFITL_1BYTE : uart.h
- UART_TLCTL_RFITL_4BYTES : uart.h
- UART_TLCTL_RFITL_8BYTES : uart.h
- UART_TLCTL_RFITL_Msk : Nano100Series.h
- UART_TLCTL_RFITL_Pos : Nano100Series.h
- UART_TLCTL_RTS_TRI_LEV_14BYTES : uart.h
- UART_TLCTL_RTS_TRI_LEV_1BYTE : uart.h
- UART_TLCTL_RTS_TRI_LEV_4BYTES : uart.h
- UART_TLCTL_RTS_TRI_LEV_8BYTES : uart.h
- UART_TLCTL_RTS_TRI_LEV_Msk : Nano100Series.h
- UART_TLCTL_RTS_TRI_LEV_Pos : Nano100Series.h
- UART_TLCTL_SPE_Msk : Nano100Series.h
- UART_TLCTL_SPE_Pos : Nano100Series.h
- UART_TMCTL_DLY_Msk : Nano100Series.h
- UART_TMCTL_DLY_Pos : Nano100Series.h
- UART_TMCTL_TOIC_Msk : Nano100Series.h
- UART_TMCTL_TOIC_Pos : Nano100Series.h
- UART_TRSR_ABAUD_F_Msk : Nano100Series.h
- UART_TRSR_ABAUD_F_Pos : Nano100Series.h
- UART_TRSR_ABAUD_TOUT_F_Msk : Nano100Series.h
- UART_TRSR_ABAUD_TOUT_F_Pos : Nano100Series.h
- UART_TRSR_BIT_ERR_F_Msk : Nano100Series.h
- UART_TRSR_BIT_ERR_F_Pos : Nano100Series.h
- UART_TRSR_LIN_RX_F_Msk : Nano100Series.h
- UART_TRSR_LIN_RX_F_Pos : Nano100Series.h
- UART_TRSR_LIN_RX_SYNC_ERR_F_Msk : Nano100Series.h
- UART_TRSR_LIN_RX_SYNC_ERR_F_Pos : Nano100Series.h
- UART_TRSR_LIN_TX_F_Msk : Nano100Series.h
- UART_TRSR_LIN_TX_F_Pos : Nano100Series.h
- UART_TRSR_RS485_ADDET_F_Msk : Nano100Series.h
- UART_TRSR_RS485_ADDET_F_Pos : Nano100Series.h
- UART_WAIT_TX_EMPTY : uart.h
- UART_WORD_LEN_5 : uart.h
- UART_WORD_LEN_6 : uart.h
- UART_WORD_LEN_7 : uart.h
- UART_WORD_LEN_8 : uart.h
- UART_WRITE : uart.h
- UNTAG_ERASE_GROUP : SDCard.h
- UNTAG_SECTOR : SDCard.h
- USBD : Nano100Series.h
- USBD_BASE : Nano100Series.h
- USBD_BUF_BASE : usbd.h
- USBD_BUFSEG_BUFSEG_Msk : Nano100Series.h
- USBD_BUFSEG_BUFSEG_Pos : Nano100Series.h
- USBD_BUSSTS_FLDET_Msk : Nano100Series.h
- USBD_BUSSTS_FLDET_Pos : Nano100Series.h
- USBD_BUSSTS_RESUME_Msk : Nano100Series.h
- USBD_BUSSTS_RESUME_Pos : Nano100Series.h
- USBD_BUSSTS_SUSPEND_Msk : Nano100Series.h
- USBD_BUSSTS_SUSPEND_Pos : Nano100Series.h
- USBD_BUSSTS_TIMEOUT_Msk : Nano100Series.h
- USBD_BUSSTS_TIMEOUT_Pos : Nano100Series.h
- USBD_BUSSTS_USBRST_Msk : Nano100Series.h
- USBD_BUSSTS_USBRST_Pos : Nano100Series.h
- USBD_CFG_CLRRDY_Msk : Nano100Series.h
- USBD_CFG_CLRRDY_Pos : Nano100Series.h
- USBD_CFG_CSTALL : usbd.h
- USBD_CFG_CSTALL_Msk : Nano100Series.h
- USBD_CFG_CSTALL_Pos : Nano100Series.h
- USBD_CFG_DSQ_SYNC_Msk : Nano100Series.h
- USBD_CFG_DSQ_SYNC_Pos : Nano100Series.h
- USBD_CFG_EP_NUM_Msk : Nano100Series.h
- USBD_CFG_EP_NUM_Pos : Nano100Series.h
- USBD_CFG_EPMODE_DISABLE : usbd.h
- USBD_CFG_EPMODE_IN : usbd.h
- USBD_CFG_EPMODE_Msk : Nano100Series.h
- USBD_CFG_EPMODE_OUT : usbd.h
- USBD_CFG_EPMODE_Pos : Nano100Series.h
- USBD_CFG_ISOCH_Msk : Nano100Series.h
- USBD_CFG_ISOCH_Pos : Nano100Series.h
- USBD_CFG_SSTALL : usbd.h
- USBD_CFG_SSTALL_Msk : Nano100Series.h
- USBD_CFG_SSTALL_Pos : Nano100Series.h
- USBD_CFG_TYPE_ISO : usbd.h
- USBD_CLR_EP_STALL : usbd.h
- USBD_CLR_INT_FLAG : usbd.h
- USBD_CLR_SE0 : usbd.h
- USBD_CONFIG_EP : usbd.h
- USBD_CTL_DPPU_EN_Msk : Nano100Series.h
- USBD_CTL_DPPU_EN_Pos : Nano100Series.h
- USBD_CTL_DRVSE0_Msk : Nano100Series.h
- USBD_CTL_DRVSE0_Pos : Nano100Series.h
- USBD_CTL_PHY_EN_Msk : Nano100Series.h
- USBD_CTL_PHY_EN_Pos : Nano100Series.h
- USBD_CTL_PWRDB_Msk : Nano100Series.h
- USBD_CTL_PWRDB_Pos : Nano100Series.h
- USBD_CTL_RWAKEUP_Msk : Nano100Series.h
- USBD_CTL_RWAKEUP_Pos : Nano100Series.h
- USBD_CTL_USB_EN_Msk : Nano100Series.h
- USBD_CTL_USB_EN_Pos : Nano100Series.h
- USBD_CTL_WAKEUP_EN_Msk : Nano100Series.h
- USBD_CTL_WAKEUP_EN_Pos : Nano100Series.h
- USBD_DISABLE_PHY : usbd.h
- USBD_DISABLE_USB : usbd.h
- USBD_DPPU_EN : usbd.h
- USBD_DRVSE0 : usbd.h
- USBD_ENABLE_INT : usbd.h
- USBD_ENABLE_PHY : usbd.h
- USBD_ENABLE_USB : usbd.h
- USBD_EPSTS2_EPSTS6_Msk : Nano100Series.h
- USBD_EPSTS2_EPSTS6_Pos : Nano100Series.h
- USBD_EPSTS2_EPSTS7_Msk : Nano100Series.h
- USBD_EPSTS2_EPSTS7_Pos : Nano100Series.h
- USBD_EPSTS_EPSTS0_Msk : Nano100Series.h
- USBD_EPSTS_EPSTS0_Pos : Nano100Series.h
- USBD_EPSTS_EPSTS1_Msk : Nano100Series.h
- USBD_EPSTS_EPSTS1_Pos : Nano100Series.h
- USBD_EPSTS_EPSTS2_Msk : Nano100Series.h
- USBD_EPSTS_EPSTS2_Pos : Nano100Series.h
- USBD_EPSTS_EPSTS3_Msk : Nano100Series.h
- USBD_EPSTS_EPSTS3_Pos : Nano100Series.h
- USBD_EPSTS_EPSTS4_Msk : Nano100Series.h
- USBD_EPSTS_EPSTS4_Pos : Nano100Series.h
- USBD_EPSTS_EPSTS5_Msk : Nano100Series.h
- USBD_EPSTS_EPSTS5_Pos : Nano100Series.h
- USBD_EPSTS_OVERRUN_Msk : Nano100Series.h
- USBD_EPSTS_OVERRUN_Pos : Nano100Series.h
- USBD_FADDR_FADDR_Msk : Nano100Series.h
- USBD_FADDR_FADDR_Pos : Nano100Series.h
- USBD_GET_ADDR : usbd.h
- USBD_GET_BUS_STATE : usbd.h
- USBD_GET_EP_BUF_ADDR : usbd.h
- USBD_GET_EP_FLAG : usbd.h
- USBD_GET_EP_STALL : usbd.h
- USBD_GET_INT_FLAG : usbd.h
- USBD_GET_PAYLOAD_LEN : usbd.h
- USBD_INT_BUS : usbd.h
- USBD_INT_FLDET : usbd.h
- USBD_INT_USB : usbd.h
- USBD_INT_WAKEUP : usbd.h
- USBD_INTEN_BUSEVT_IE_Msk : Nano100Series.h
- USBD_INTEN_BUSEVT_IE_Pos : Nano100Series.h
- USBD_INTEN_FLDET_IE_Msk : Nano100Series.h
- USBD_INTEN_FLDET_IE_Pos : Nano100Series.h
- USBD_INTEN_USBEVT_IE_Msk : Nano100Series.h
- USBD_INTEN_USBEVT_IE_Pos : Nano100Series.h
- USBD_INTEN_WAKEUP_IE_Msk : Nano100Series.h
- USBD_INTEN_WAKEUP_IE_Pos : Nano100Series.h
- USBD_INTSTS_BUS : usbd.h
- USBD_INTSTS_BUS_STS_Msk : Nano100Series.h
- USBD_INTSTS_BUS_STS_Pos : Nano100Series.h
- USBD_INTSTS_EP0 : usbd.h
- USBD_INTSTS_EP1 : usbd.h
- USBD_INTSTS_EP2 : usbd.h
- USBD_INTSTS_EP3 : usbd.h
- USBD_INTSTS_EP4 : usbd.h
- USBD_INTSTS_EP5 : usbd.h
- USBD_INTSTS_EP6 : usbd.h
- USBD_INTSTS_EP7 : usbd.h
- USBD_INTSTS_EPEVT0_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT0_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT1_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT1_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT2_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT2_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT3_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT3_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT4_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT4_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT5_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT5_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT6_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT6_Pos : Nano100Series.h
- USBD_INTSTS_EPEVT7_Msk : Nano100Series.h
- USBD_INTSTS_EPEVT7_Pos : Nano100Series.h
- USBD_INTSTS_FLD_STS_Msk : Nano100Series.h
- USBD_INTSTS_FLD_STS_Pos : Nano100Series.h
- USBD_INTSTS_FLDET : usbd.h
- USBD_INTSTS_SETUP : usbd.h
- USBD_INTSTS_SETUP_Msk : Nano100Series.h
- USBD_INTSTS_SETUP_Pos : Nano100Series.h
- USBD_INTSTS_USB : usbd.h
- USBD_INTSTS_USB_STS_Msk : Nano100Series.h
- USBD_INTSTS_USB_STS_Pos : Nano100Series.h
- USBD_INTSTS_WAKEUP : usbd.h
- USBD_INTSTS_WKEUP_STS_Msk : Nano100Series.h
- USBD_INTSTS_WKEUP_STS_Pos : Nano100Series.h
- USBD_IS_ATTACHED : usbd.h
- USBD_MAX_EP : usbd.h
- USBD_MODULE : clk.h
- USBD_MXPLD_MXPLD_Msk : Nano100Series.h
- USBD_MXPLD_MXPLD_Pos : Nano100Series.h
- USBD_PDMA_BYTEM_Msk : Nano100Series.h
- USBD_PDMA_BYTEM_Pos : Nano100Series.h
- USBD_PDMA_PDMA_RST_Msk : Nano100Series.h
- USBD_PDMA_PDMA_RST_Pos : Nano100Series.h
- USBD_PDMA_PDMA_RW_Msk : Nano100Series.h
- USBD_PDMA_PDMA_RW_Pos : Nano100Series.h
- USBD_PDMA_PDMA_TRG_Msk : Nano100Series.h
- USBD_PDMA_PDMA_TRG_Pos : Nano100Series.h
- USBD_PHY_EN : usbd.h
- USBD_PWRDN : usbd.h
- USBD_RST : sys.h
- USBD_SET_ADDR : usbd.h
- USBD_SET_DATA0 : usbd.h
- USBD_SET_DATA1 : usbd.h
- USBD_SET_EP_BUF_ADDR : usbd.h
- USBD_SET_EP_STALL : usbd.h
- USBD_SET_PAYLOAD_LEN : usbd.h
- USBD_SET_SE0 : usbd.h
- USBD_STATE_RESUME : usbd.h
- USBD_STATE_SUSPEND : usbd.h
- USBD_STATE_TIMEOUT : usbd.h
- USBD_STATE_USBRST : usbd.h
- USBD_STOP_TRANSACTION : usbd.h
- USBD_USB_EN : usbd.h
- USBD_WAKEUP_EN : usbd.h