| Airoha M0 BLE API 1.0.5.4

Data Fields
GATT_4_8_4_PARA Struct Reference
ble_gatt_client.h

GATT Client API parameter for ble_gatt_4_8_4_read_multi_char_values. More...

## Data Fields
uint16_t | conn_handle
| connection handle of designated gatt server
uint8_t | numofhandles
| number of handles to be read
uint16_t | att_handle [5]
| array of attribute handles to be read

## Detailed Description

GATT Client API parameter for ble_gatt_4_8_4_read_multi_char_values.