| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

Functions
NuEdu-Basic01_I2C_EEPROM.h File Reference

NuEdu-Basic01_I2C_EEPROM I2C driver header file for NuEdu-SDK-Nano130. More...

`#include "Nano100Series.h"`

Go to the source code of this file.

## Functions
void | I2C_EEPROM_Init (uint8_t u8Divider)
| This function initializes the I2C module, bit-rate = 100 kHz and enable the corresponding interrupt. More...
void | I2C_EEPROM_Write (uint16_t u16Address, uint8_t u8Data)
| This function do the I2C data writing to EEPROM device. More...
uint8_t | I2C_EEPROM_Read (uint16_t u16Address)
| This function do the I2C data reading from EEPROM device. More...

## Detailed Description

NuEdu-Basic01_I2C_EEPROM I2C driver header file for NuEdu-SDK-Nano130.

Version
  V1.00

Revision
  4

Date
  14/10/17 4:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013-2014 Nuvoton Technology Corp. All rights reserved.

Definition in file NuEdu-Basic01_I2C_EEPROM.h.