| Airoha M0 BLE API 1.0.5.4

Data Fields
PPCP_t Struct Reference
service_generic_access.h

Peripheral Preferred Connection Parameters. More...

## Data Fields
uint16_t | min_interval
uint16_t | max_interval
uint16_t | slave_latency
uint16_t | supervision_TO

## Detailed Description

Peripheral Preferred Connection Parameters.

## Field Documentation

## ◆ min_interval

uint16_t PPCP_t::min_interval

Connection Interval = min_interval* 1.25 ms range: 6~3200 ;65535=no specific minimum

## ◆ max_interval

uint16_t PPCP_t::max_interval

Connection Interval = max_interval* 1.25 ms range: 6~3200 ;65535=no specific minimum

## ◆ slave_latency

uint16_t PPCP_t::slave_latency

range: 0~1000

## ◆ supervision_TO

uint16_t PPCP_t::supervision_TO

Connection Supervision Timeout Multiplier range:10~3200 ;65535=no specific value requested