| Nano100BN Series BSP V3.03.002 The Board Support Package for Nano100BN Series

NuEdu-Basic01_Button.h
Go to the documentation of this file.
1 /**************************************************************************/
12 #ifndef __NuEdu_Basic01_Button_H__
13 #define __NuEdu_Basic01_Button_H__
14
26 /*---------------------------------------------------------------------------------------------------------*/
27 /* Functions */
28 /*---------------------------------------------------------------------------------------------------------*/
29 extern void Initial_KEY_INPUT(void);
30 extern unsigned char Get_KEY_INPUT(void);
31
32 #endif
33 /* end of group Nano130_Basic01_FUNCTIONS */
34 /* end of group NuEdu-SDK-Nano130_Basic01 */
36 /* end of group NANO100_Library */
38
39 /*** (C) COPYRIGHT 2013-2014 Nuvoton Technology Corp. ***/
Initial_KEY_INPUT
void Initial_KEY_INPUT(void)
Set Button GPIO to input mode.
Definition: NuEdu-Basic01_Button.c:37
Get_KEY_INPUT
unsigned char Get_KEY_INPUT(void)
This function get button status.
Definition: NuEdu-Basic01_Button.c:48