| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gap_evt_remote_version_t Struct Reference
ble_gap.h

Event structure for BLE_GAP_EVT_READ_REMOTE_VERSION. More...

## Data Fields
uint8_t | err_code
| HCI error code.
uint16_t | handle
| Connection handle.
uint8_t | version
| Version of current LMP.
uint16_t | manu
| Manufacturer name.
uint16_t | sub
| Subversion.

## Detailed Description

Event structure for BLE_GAP_EVT_READ_REMOTE_VERSION.