| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gap_scan_params_t Struct Reference
ble_gap.h

Parameter for scanning. More...

## Data Fields
uint16_t | interval
| Scan interval between 0x0004 and 0x4000 in 0.625ms units (2.5ms to 10.24s).
uint16_t | window
| Scan window between 0x0004 and 0x4000 in 0.625ms units (2.5ms to 10.24s).
ble_scan_policy_t | policy
ble_gap_whitelist_t * | p_whitelist
| Pointer to whitelist, NULL if no whitelist or the current active whitelist is to be used.
bool | filter_duplicated
| Filter duplicated device.

## Detailed Description

Parameter for scanning.

## Field Documentation

## ◆ policy

ble_scan_policy_t ble_gap_scan_params_t::policy

! Owner address type