| Airoha M0 BLE API 1.0.5.4

Data Fields
ble_gap_create_conn_params_t Struct Reference
ble_gap.h

parameters for creating a link More...

## Data Fields
uint16_t | scan_intvl
| Scan interval between 0x0004 and 0x4000 in 0.625ms units (2.5ms to 10.24s).
uint16_t | scan_window
| Scan window between 0x0004 and 0x4000 in 0.625ms units (2.5ms to 10.24s).
ble_addr_type | owner
uint16_t | min_conn_interval
| Minimum Connection Interval in 1.25 ms units,. More...
uint16_t | max_conn_interval
| Maximum Connection Interval in 1.25 ms units,.
uint16_t | slave_latency
| Slave Latency in number of connection events.
uint16_t | conn_sup_timeout
| Connection Supervision Timeout in 10 ms units.
uint16_t | ce_min
| Minimal CE.
uint16_t | ce_max
| Maximal CE.

## Detailed Description

parameters for creating a link

## Field Documentation

## ◆ owner

ble_addr_type ble_gap_create_conn_params_t::owner

! peer address

## ◆ min_conn_interval

uint16_t ble_gap_create_conn_params_t::min_conn_interval

Minimum Connection Interval in 1.25 ms units,.

! owner address