| Nano102_112 Series BSP V3.03.002 The Board Support Package for Nano102_112 Series

Data Fields
S_RTC_TIME_DATA_T Struct Reference
NANO102/112 Device Driver » RTC Driver » RTC Exported Structs

RTC define Time Data Struct. More...

`#include <rtc.h>`

## Data Fields
uint32_t | u32Year
uint32_t | u32Month
uint32_t | u32Day
uint32_t | u32DayOfWeek
uint32_t | u32Hour
uint32_t | u32Minute
uint32_t | u32Second
uint32_t | u32TimeScale
uint32_t | u32AmPm

## Detailed Description

RTC define Time Data Struct.

Definition at line 81 of file rtc.h.

## Field Documentation

## ◆ u32AmPm

uint32_t S_RTC_TIME_DATA_T::u32AmPm

Only Time Scale select 12-hr used

Definition at line 90 of file rtc.h.

## ◆ u32Day

uint32_t S_RTC_TIME_DATA_T::u32Day

Day value

Definition at line 84 of file rtc.h.

## ◆ u32DayOfWeek

uint32_t S_RTC_TIME_DATA_T::u32DayOfWeek

Day of week value

Definition at line 85 of file rtc.h.

## ◆ u32Hour

uint32_t S_RTC_TIME_DATA_T::u32Hour

Hour value

Definition at line 86 of file rtc.h.

## ◆ u32Minute

uint32_t S_RTC_TIME_DATA_T::u32Minute

Minute value

Definition at line 87 of file rtc.h.

## ◆ u32Month

uint32_t S_RTC_TIME_DATA_T::u32Month

Month value

Definition at line 83 of file rtc.h.

## ◆ u32Second

uint32_t S_RTC_TIME_DATA_T::u32Second

Second value

Definition at line 88 of file rtc.h.

## ◆ u32TimeScale

uint32_t S_RTC_TIME_DATA_T::u32TimeScale

12-Hour, 24-Hour

Definition at line 89 of file rtc.h.

## ◆ u32Year

uint32_t S_RTC_TIME_DATA_T::u32Year

Year value

Definition at line 82 of file rtc.h.

The documentation for this struct was generated from the following file:

- StdDriver/inc/rtc.h