| Nano102_112 Series BSP V3.03.002 The Board Support Package for Nano102_112 Series

Macros
SYS Exported Constants
NANO102/112 Device Driver » SYS Driver

## Macros
#define | CPU_RST ((0x0<<24) | SYS_IPRST_CTL1_CPU_RST_Pos )
#define | CHIP_RST ((0x0<<24) | SYS_IPRST_CTL1_CHIP_RST_Pos )
#define | DMA_RST ((0x0<<24) | SYS_IPRST_CTL1_DMA_RST_Pos )
#define | SC1_RST ((0x4<<24) | SYS_IPRST_CTL2_SC1_RST_Pos )
#define | SC0_RST ((0x4<<24) | SYS_IPRST_CTL2_SC0_RST_Pos )
#define | ADC_RST ((0x4<<24) | SYS_IPRST_CTL2_ADC_RST_Pos )
#define | LCD_RST ((0x4<<24) | SYS_IPRST_CTL2_LCD_RST_Pos )
#define | ACMP01_RST ((0x4<<24) | SYS_IPRST_CTL2_ACMP01_RST_Pos )
#define | PWM0_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM0_RST_Pos )
#define | UART1_RST ((0x4<<24) | SYS_IPRST_CTL2_UART1_RST_Pos )
#define | UART0_RST ((0x4<<24) | SYS_IPRST_CTL2_UART0_RST_Pos )
#define | SPI1_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI1_RST_Pos )
#define | SPI0_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI0_RST_Pos )
#define | I2C1_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C1_RST_Pos )
#define | I2C0_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C0_RST_Pos )
#define | TMR3_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR3_RST_Pos )
#define | TMR2_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR2_RST_Pos )
#define | TMR1_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR1_RST_Pos )
#define | TMR0_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR0_RST_Pos )
#define | GPIO_RST ((0x4<<24) | SYS_IPRST_CTL2_GPIO_RST_Pos )
#define | SYS_VREFCTL_BGP_EN ((uint32_t)0x00000001)
#define | SYS_VREFCTL_REG_EN ((uint32_t)0x00000002)
#define | SYS_VREFCTL_SEL25 ((uint32_t)0x00000008)
#define | SYS_VREFCTL_SEL18 ((uint32_t)0x00000004)
#define | SYS_VREFCTL_SEL15 ((uint32_t)0x00000000)
#define | SYS_VREFCTL_EXTMODE ((uint32_t)0x00000010)
#define | SYS_LDOCTL_LDO_PD ((uint32_t)0x00000001)
#define | SYS_LDOCTL_LDO_LEVEL16 ((uint32_t)0x00000004)
#define | SYS_LDOCTL_LDO_LEVEL18 ((uint32_t)0x00000008)
#define | SYS_IRCTRIMCTL_TRIM_11_0592M ((uint32_t)0x00000001)
#define | SYS_IRCTRIMCTL_TRIM_12M ((uint32_t)0x00000002)
#define | SYS_IRCTRIMCTL_TRIM_16M ((uint32_t)0x00000003)
#define | SYS_IRCTRIMCTL_LOOP_4CLK ((uint32_t)0x00000000)
#define | SYS_IRCTRIMCTL_LOOP_8CLK ((uint32_t)0x00000010)
#define | SYS_IRCTRIMCTL_LOOP_16CLK ((uint32_t)0x00000020)
#define | SYS_IRCTRIMCTL_LOOP_32CLK ((uint32_t)0x00000030)
#define | SYS_IRCTRIMCTL_RETRY_64 ((uint32_t)0x00000000)
#define | SYS_IRCTRIMCTL_RETRY_128 ((uint32_t)0x00000040)
#define | SYS_IRCTRIMCTL_RETRY_256 ((uint32_t)0x00000080)
#define | SYS_IRCTRIMCTL_RETRY_512 ((uint32_t)0x000000C0)
#define | SYS_IRCTRIMCTL_CLKERR_STOP ((uint32_t)0x00000100)
#define | SYS_IRCTRIMIEN_DISABLE ((uint32_t)0x00000000)
#define | SYS_IRCTRIMIEN_FAIL_EN ((uint32_t)0x00000002)
#define | SYS_IRCTRIMIEN_32KERR_EN ((uint32_t)0x00000004)
#define | SYS_IRCTRIMINT_FREQLOCK ((uint32_t)0x00000001)
#define | SYS_IRCTRIMINT_FAIL_INT ((uint32_t)0x00000002)
#define | SYS_IRCTRIMINT_32KERR_INT ((uint32_t)0x00000004)
#define | SYS_PA_L_MFP_PA7_MFP_GPA7 (0UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_ADC_CH7 (2UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA7_MFP_SC1_CD (4UL<<SYS_PA_L_MFP_PA7_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_GPA6 (0UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_ADC_CH6 (2UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_ACMP0_O (3UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_SC0_RST (4UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA6_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA6_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_GPA5 (0UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_ADC_CH5 (2UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_ACMP0_N (3UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_SC0_PWR (4UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_I2C1_SDA (5UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_SPI1_SS0 (6UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA5_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA5_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_GPA4 (0UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_ADC_CH4 (2UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_SC0_CD (4UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA4_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA4_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_GPA3 (0UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_EINT1 (1UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_ADC_CH3 (2UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_SC0_DAT (4UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA3_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA3_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_GPA2 (0UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_EINT0 (1UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_ADC_CH2 (2UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_SC0_CLK (4UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA2_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA2_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_GPA1 (0UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_ADC_CH1 (2UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA1_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA1_MFP_Pos)
#define | SYS_PA_L_MFP_PA0_MFP_GPA0 (0UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
#define | SYS_PA_L_MFP_PA0_MFP_ADC_CH0 (2UL<<SYS_PA_L_MFP_PA0_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_GPA15 (0UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_TMR3_CAP (2UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_ACMP1_O (3UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_I2C1_SDA (5UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_SPI1_SS0 (6UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_LCD_S16 (8UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA15_MFP_LCD_S30 (8UL<<SYS_PA_H_MFP_PA15_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_GPA14 (0UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_I2C1_SCL (5UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_SPI1_SCLK (6UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_LCD_S17 (8UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_LCD_S31 (8UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA14_MFP_ACMP0_C (9UL<<SYS_PA_H_MFP_PA14_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_GPA13 (0UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_ACMP1_N (3UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_I2C0_SDA (5UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_SPI1_MISO0 (6UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_UART0_RX (7UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA13_MFP_LCD_S18 (8UL<<SYS_PA_H_MFP_PA13_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_GPA12 (0UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_ACMP1_P (3UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_I2C0_SCL (5UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_SPI1_MOSI0 (6UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_UART0_TX (7UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA12_MFP_LCD_S19 (8UL<<SYS_PA_H_MFP_PA12_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_GPA11 (0UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_ADC_EXT (2UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA11_MFP_SC0_DAT (4UL<<SYS_PA_H_MFP_PA11_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_GPA10 (0UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA10_MFP_SC0_CLK (4UL<<SYS_PA_H_MFP_PA10_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_GPA9 (0UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA9_MFP_SC0_RST (4UL<<SYS_PA_H_MFP_PA9_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_GPA8 (0UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PA_H_MFP_PA8_MFP_SC0_PWR (4UL<<SYS_PA_H_MFP_PA8_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_GPB7 (0UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_SC0_CD (4UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_UART1_CTS (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB7_MFP_LCD_S33 (8UL<<SYS_PB_L_MFP_PB7_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_GPB6 (0UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_CKO0 (1UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_SPI1_SS1 (6UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_UART1_TX (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_LCD_S25 (8UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB6_MFP_LCD_S34 (8UL<<SYS_PB_L_MFP_PB6_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_GPB5 (0UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_SPI1_MOSI1 (6UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_UART1_RX (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB5_MFP_LCD_S35 (8UL<<SYS_PB_L_MFP_PB5_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_GPB4 (0UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_SPI1_MISO1 (6UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB4_MFP_UART1_RTS (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_GPB3 (0UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_TMR2_CNT (2UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_I2C0_SDA (5UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_SPI1_MISO1 (6UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_UART0_CTS (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_LCD_S26 (8UL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB3_MFP_TMR2_OUT (0xAUL<<SYS_PB_L_MFP_PB3_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_GPB2 (0UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_TMR3_CNT (2UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_I2C0_SCL (5UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_SPI1_MOSI1 (6UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_UART0_RTS (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_LCD_S27 (8UL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB2_MFP_TMR3_OUT (0xAUL<<SYS_PB_L_MFP_PB2_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_GPB1 (0UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_EINT1 (1UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_TMR2_CAP (2UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_UART0_RX (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB1_MFP_LCD_S28 (8UL<<SYS_PB_L_MFP_PB1_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_GPB0 (0UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_CKO1 (1UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_UART0_TX (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_L_MFP_PB0_MFP_LCD_S29 (8UL<<SYS_PB_L_MFP_PB0_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_GPB15 (0UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_SPI0_SS0 (6UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_UART0_CTS (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_LCD_S12 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_LCD_S19 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB15_MFP_LCD_S23 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_GPB14 (0UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_SPI0_SCLK (6UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_UART0_TX (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_LCD_S13 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_LCD_S20 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB14_MFP_LCD_S24 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_GPB13 (0UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_SPI0_MISO0 (6UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_UART0_RX (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_LCD_S14 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_LCD_S21 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB13_MFP_LCD_S25 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_GPB12 (0UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_CKO0 (1UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_TMR0_CNT (2UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_SPI0_MOSI0 (6UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_UART0_RTS (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_LCD_S15 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_LCD_S22 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_LCD_S26 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB12_MFP_TMR0_OUT (0xAUL<<SYS_PB_H_MFP_PB12_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_GPB11 (0UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_TMR1_CNT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_SPI0_MISO1 (6UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_UART1_RTS (7UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_LCD_S23 (8UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_LCD_S27 (8UL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB11_MFP_TMR1_OUT (0xAUL<<SYS_PB_H_MFP_PB11_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_GPB10 (0UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI1 (6UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_UART1_RX (7UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_LCD_S24 (8UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB10_MFP_LCD_S28 (8UL<<SYS_PB_H_MFP_PB10_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_GPB9 (0UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_PWM0_CH1 (3UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB9_MFP_LCD_S31 (8UL<<SYS_PB_H_MFP_PB9_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_GPB8 (0UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_EINT1 (1UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_TMR0_CNT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_PWM0_CH0 (3UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_SNOOPER (4UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_LCD_S32 (8UL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PB_H_MFP_PB8_MFP_TMR0_OUT (0xAUL<<SYS_PB_H_MFP_PB8_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_GPC7 (0UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_SC0_PWR (4UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_UART1_RX (7UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_LCD_S4 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_LCD_S11 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC7_MFP_LCD_S15 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_GPC6 (0UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_SC0_DAT (4UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_UART1_RTS (7UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_LCD_S5 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_LCD_S12 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC6_MFP_LCD_S16 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_GPC5 (0UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_SC0_CD (4UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_LCD_S6 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_LCD_S13 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC5_MFP_LCD_S17 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_GPC4 (0UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_EINT0 (1UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_SC0_CLK (4UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_UART1_CTS (7UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_LCD_S7 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_LCD_S14 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC4_MFP_LCD_S18 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_GPC3 (0UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_PWM0_CH3 (3UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_I2C1_SDA (5UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_LCD_S8 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_LCD_S15 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC3_MFP_LCD_S19 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_GPC2 (0UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_PWM0_CH2 (3UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_I2C1_SCL (5UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_LCD_S9 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_LCD_S16 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC2_MFP_LCD_S20 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_GPC1 (0UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_PWM0_CH1 (3UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_I2C0_SDA (5UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_LCD_S10 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_LCD_S17 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC1_MFP_LCD_S21 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_GPC0 (0UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_PWM0_CH0 (3UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_I2C0_SCL (5UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_SPI0_SS1 (6UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_LCD_S11 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_LCD_S18 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_L_MFP_PC0_MFP_LCD_S22 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_GPC15 (0UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_SC1_PWR (4UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_LCD_S0 (8UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC15_MFP_LCD_S7 (8UL<<SYS_PC_H_MFP_PC15_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_GPC14 (0UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_SC1_CD (4UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_LCD_S1 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC14_MFP_LCD_S8 (8UL<<SYS_PC_H_MFP_PC14_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_GPC13 (0UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_SC1_DAT (4UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC13_MFP_LCD_S9 (8UL<<SYS_PC_H_MFP_PC13_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_GPC12 (0UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_SC1_CLK (4UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC12_MFP_LCD_S10 (8UL<<SYS_PC_H_MFP_PC12_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_GPC11 (0UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_SC1_PWR (4UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_I2C1_SDA (5UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC11_MFP_LCD_S11 (8UL<<SYS_PC_H_MFP_PC11_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_GPC10 (0UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_SC1_CD (4UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_I2C1_SCL (5UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC10_MFP_LCD_S12 (8UL<<SYS_PC_H_MFP_PC10_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_GPC9 (0UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_LCD_S2 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_LCD_S9 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC9_MFP_LCD_S13 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_GPC8 (0UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_SC0_RST (4UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_UART1_TX (7UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_LCD_S3 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_LCD_S10 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PC_H_MFP_PC8_MFP_LCD_S14 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)
#define | SYS_PD_L_MFP_PD7_MFP_GPD7 (0UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
#define | SYS_PD_L_MFP_PD7_MFP_SC1_CLK (4UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
#define | SYS_PD_L_MFP_PD7_MFP_LCD_COM3 (8UL<<SYS_PD_L_MFP_PD7_MFP_Pos)
#define | SYS_PD_L_MFP_PD6_MFP_GPD6 (0UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
#define | SYS_PD_L_MFP_PD6_MFP_LCD_S0 (8UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
#define | SYS_PD_L_MFP_PD6_MFP_LCD_COM4 (8UL<<SYS_PD_L_MFP_PD6_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_GPD5 (0UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_LCD_S1 (8UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD5_MFP_LCD_COM5 (8UL<<SYS_PD_L_MFP_PD5_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_GPD4 (0UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_SC1_RST (4UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD4_MFP_LCD_S2 (8UL<<SYS_PD_L_MFP_PD4_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_GPD3 (0UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD3_MFP_LCD_S3 (8UL<<SYS_PD_L_MFP_PD3_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_GPD2 (0UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD2_MFP_LCD_S4 (8UL<<SYS_PD_L_MFP_PD2_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_GPD1 (0UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD1_MFP_LCD_S5 (8UL<<SYS_PD_L_MFP_PD1_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_GPD0 (0UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_L_MFP_PD0_MFP_LCD_S6 (8UL<<SYS_PD_L_MFP_PD0_MFP_Pos)
#define | SYS_PD_H_MFP_PD15_MFP_GPD15 (0UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
#define | SYS_PD_H_MFP_PD15_MFP_LCD_V3 (8UL<<SYS_PD_H_MFP_PD15_MFP_Pos)
#define | SYS_PD_H_MFP_PD14_MFP_GPD14 (0UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
#define | SYS_PD_H_MFP_PD14_MFP_LCD_V2 (8UL<<SYS_PD_H_MFP_PD14_MFP_Pos)
#define | SYS_PD_H_MFP_PD13_MFP_GPD13 (0UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
#define | SYS_PD_H_MFP_PD13_MFP_EINT1 (1UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
#define | SYS_PD_H_MFP_PD13_MFP_LCD_V1 (8UL<<SYS_PD_H_MFP_PD13_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_GPD12 (0UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_CKO0 (1UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_TMR1_CNT (2UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_PWM0_CH0 (3UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_LCD_DH1 (8UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_CLK_Hz (9UL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD12_MFP_TMR1_OUT (0xAUL<<SYS_PD_H_MFP_PD12_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_GPD11 (0UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_TMR0_CAP (2UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_PWM0_CH1 (3UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD11_MFP_LCD_DH2 (8UL<<SYS_PD_H_MFP_PD11_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_GPD10 (0UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_TMR1_CAP (2UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_PWM0_CH2 (3UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD10_MFP_LCD_COM0 (8UL<<SYS_PD_H_MFP_PD10_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_GPD9 (0UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_PWM0_CH3 (3UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_SC1_RST (4UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD9_MFP_LCD_COM1 (8UL<<SYS_PD_H_MFP_PD9_MFP_Pos)
#define | SYS_PD_H_MFP_PD8_MFP_GPD8 (0UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
#define | SYS_PD_H_MFP_PD8_MFP_SC1_DAT (4UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
#define | SYS_PD_H_MFP_PD8_MFP_LCD_COM2 (8UL<<SYS_PD_H_MFP_PD8_MFP_Pos)
#define | SYS_PE_L_MFP_PE7_MFP_GPE7 (0UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
#define | SYS_PE_L_MFP_PE7_MFP_SC1_DAT (4UL<<SYS_PE_L_MFP_PE7_MFP_Pos)
#define | SYS_PE_L_MFP_PE6_MFP_GPE6 (0UL<<SYS_PE_L_MFP_PE6_MFP_Pos)
#define | SYS_PE_L_MFP_PE6_MFP_SC1_CLK (4UL<<SYS_PE_L_MFP_PE6_MFP_Pos)
#define | SYS_PE_L_MFP_PE5_MFP_GPE5 (0UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
#define | SYS_PE_L_MFP_PE5_MFP_SC1_PWR (4UL<<SYS_PE_L_MFP_PE5_MFP_Pos)
#define | SYS_PE_L_MFP_PE4_MFP_GPE4 (0UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
#define | SYS_PE_L_MFP_PE4_MFP_SC1_RST (4UL<<SYS_PE_L_MFP_PE4_MFP_Pos)
#define | SYS_PE_L_MFP_PE3_MFP_GPE3 (0UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
#define | SYS_PE_L_MFP_PE3_MFP_SPI0_SS0 (6UL<<SYS_PE_L_MFP_PE3_MFP_Pos)
#define | SYS_PE_L_MFP_PE2_MFP_GPE2 (0UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
#define | SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK (6UL<<SYS_PE_L_MFP_PE2_MFP_Pos)
#define | SYS_PE_L_MFP_PE1_MFP_GPE1 (0UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
#define | SYS_PE_L_MFP_PE1_MFP_SPI0_MISO0 (6UL<<SYS_PE_L_MFP_PE1_MFP_Pos)
#define | SYS_PE_L_MFP_PE0_MFP_GPE0 (0UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
#define | SYS_PE_L_MFP_PE0_MFP_SPI0_MOSI0 (6UL<<SYS_PE_L_MFP_PE0_MFP_Pos)
#define | SYS_PE_H_MFP_PE9_MFP_GPE9 (0UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
#define | SYS_PE_H_MFP_PE9_MFP_PWM0_CH3 (3UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
#define | SYS_PE_H_MFP_PE9_MFP_LCD_S29 (8UL<<SYS_PE_H_MFP_PE9_MFP_Pos)
#define | SYS_PE_H_MFP_PE8_MFP_GPE8 (0UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
#define | SYS_PE_H_MFP_PE8_MFP_PWM0_CH2 (3UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
#define | SYS_PE_H_MFP_PE8_MFP_LCD_S30 (8UL<<SYS_PE_H_MFP_PE8_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_GPF5 (0UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_TMR0_CAP (2UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_PWM0_CH3 (3UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_ACMP_C (9UL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF5_MFP_ICE_DAT (0xFUL<<SYS_PF_L_MFP_PF5_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_GPF4 (0UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_CKO1 (1UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_TMR1_CAP (2UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_PWM0_CH2 (3UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_CLK_Hz (9UL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF4_MFP_ICE_CLK (0xFUL<<SYS_PF_L_MFP_PF4_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_GPF3 (0UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_EINT0 (1UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_TMR2_CAP (2UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_UART1_TX (7UL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF3_MFP_XT1_OUT (0xFUL<<SYS_PF_L_MFP_PF3_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_GPF2 (0UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_EINT1 (1UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_TMR3_CAP (2UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_UART1_RX (7UL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF2_MFP_XT1_IN (0xFUL<<SYS_PF_L_MFP_PF2_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_GPF1 (0UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_TMR2_CNT (2UL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_X32_OUT (0xFUL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF1_MFP_TMR2_OUT (0xAUL<<SYS_PF_L_MFP_PF1_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_GPF0 (0UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_TMR3_CNT (2UL<<SYS_PF_L_MFP_PF0_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_X32_IN (0xFUL<<SYS_PF_L_MFP_PF0_MFP_Pos)
#define | SYS_PF_L_MFP_PF0_MFP_TMR3_OUT (0xAUL<<SYS_PF_L_MFP_PF0_MFP_Pos)
#define | MFP_LCD_TYPEA()

## Detailed Description

## Macro Definition Documentation

## ◆ ACMP01_RST

#define ACMP01_RST ((0x4<<24) | SYS_IPRST_CTL2_ACMP01_RST_Pos )

ACMP01 reset is one of the SYS_ResetModule parameter

Definition at line 42 of file sys.h.

## ◆ ADC_RST

#define ADC_RST ((0x4<<24) | SYS_IPRST_CTL2_ADC_RST_Pos )

ADC reset is one of the SYS_ResetModule parameter

Definition at line 40 of file sys.h.

## ◆ CHIP_RST

#define CHIP_RST ((0x0<<24) | SYS_IPRST_CTL1_CHIP_RST_Pos )

CHIP reset is one of the SYS_ResetModule parameter

Definition at line 36 of file sys.h.

## ◆ CPU_RST

#define CPU_RST ((0x0<<24) | SYS_IPRST_CTL1_CPU_RST_Pos )

CPU reset is one of the SYS_ResetModule parameter

Definition at line 35 of file sys.h.

## ◆ DMA_RST

#define DMA_RST ((0x0<<24) | SYS_IPRST_CTL1_DMA_RST_Pos )

DMA reset is one of the SYS_ResetModule parameter

Definition at line 37 of file sys.h.

## ◆ GPIO_RST

#define GPIO_RST ((0x4<<24) | SYS_IPRST_CTL2_GPIO_RST_Pos )

GPIO reset is one of the SYS_ResetModule parameter

Definition at line 54 of file sys.h.

## ◆ I2C0_RST

#define I2C0_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C0_RST_Pos )

I2C0 reset is one of the SYS_ResetModule parameter

Definition at line 49 of file sys.h.

## ◆ I2C1_RST

#define I2C1_RST ((0x4<<24) | SYS_IPRST_CTL2_I2C1_RST_Pos )

I2C1 reset is one of the SYS_ResetModule parameter

Definition at line 48 of file sys.h.

## ◆ LCD_RST

#define LCD_RST ((0x4<<24) | SYS_IPRST_CTL2_LCD_RST_Pos )

LCD reset is one of the SYS_ResetModule parameter

Definition at line 41 of file sys.h.

## ◆ MFP_LCD_TYPEA

#define MFP_LCD_TYPEA | ( |  | ) |

Value:
{ \
SYS->PB_L_MFP = (SYS->PB_L_MFP &~(0xFFF00000)) | (0x88800000); /* seg 35 ~ 33 */\
SYS->PB_H_MFP = 0x88888888; /* seg 32 ~ 31, 28 ~ 23 */\
SYS->PC_L_MFP = 0x88888888; /* seg 22 ~ 15 */\
SYS->PC_H_MFP = 0x88888888; /* seg 14 ~ 7 */\
SYS->PD_L_MFP = 0x88888888; /* seg 6 ~ 0, COM3 */\
SYS->PD_H_MFP = 0x88888888; /* COM2 ~ 0, DH2 ~ 1, V3 ~1 */\
SYS->PE_H_MFP = (SYS->PE_H_MFP &~(0x000000FF)) | (0x00000088); /* seg 30, 29 */\
PB->OFFD |= 0xFFE00000;\
PC->OFFD |= 0xFFFF0000;\
PD->OFFD |= 0xFFFF0000;\
PE->OFFD |= 0x03000000;\
}
SYS
#define SYS
Pointer to SYS register structure.
Definition: Nano1X2Series.h:10650

Definition at line 538 of file sys.h.

## ◆ PWM0_RST

#define PWM0_RST ((0x4<<24) | SYS_IPRST_CTL2_PWM0_RST_Pos )

PWM0 reset is one of the SYS_ResetModule parameter

Definition at line 43 of file sys.h.

## ◆ SC0_RST

#define SC0_RST ((0x4<<24) | SYS_IPRST_CTL2_SC0_RST_Pos )

SmartCard0 reset is one of the SYS_ResetModule parameter

Definition at line 39 of file sys.h.

## ◆ SC1_RST

#define SC1_RST ((0x4<<24) | SYS_IPRST_CTL2_SC1_RST_Pos )

SmartCard1 reset is one of the SYS_ResetModule parameter

Definition at line 38 of file sys.h.

## ◆ SPI0_RST

#define SPI0_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI0_RST_Pos )

SPI0 reset is one of the SYS_ResetModule parameter

Definition at line 47 of file sys.h.

## ◆ SPI1_RST

#define SPI1_RST ((0x4<<24) | SYS_IPRST_CTL2_SPI1_RST_Pos )

SPI1 reset is one of the SYS_ResetModule parameter

Definition at line 46 of file sys.h.

## ◆ SYS_IRCTRIMCTL_CLKERR_STOP

#define SYS_IRCTRIMCTL_CLKERR_STOP ((uint32_t)0x00000100)

Clock error stop enable

Definition at line 90 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_16CLK

#define SYS_IRCTRIMCTL_LOOP_16CLK ((uint32_t)0x00000020)

Based on average difference in 16 x 32.768 kHz clock

Definition at line 82 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_32CLK

#define SYS_IRCTRIMCTL_LOOP_32CLK ((uint32_t)0x00000030)

Based on average difference in 32 x 32.768 kHz clock

Definition at line 83 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_4CLK

#define SYS_IRCTRIMCTL_LOOP_4CLK ((uint32_t)0x00000000)

Based on average difference in 4 x 32.768 kHz clock

Definition at line 80 of file sys.h.

## ◆ SYS_IRCTRIMCTL_LOOP_8CLK

#define SYS_IRCTRIMCTL_LOOP_8CLK ((uint32_t)0x00000010)

Based on average difference in 8 x 32.768 kHz clock

Definition at line 81 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_128

#define SYS_IRCTRIMCTL_RETRY_128 ((uint32_t)0x00000040)

Trim retry count limitation is 128

Definition at line 86 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_256

#define SYS_IRCTRIMCTL_RETRY_256 ((uint32_t)0x00000080)

Trim retry count limitation is 256

Definition at line 87 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_512

#define SYS_IRCTRIMCTL_RETRY_512 ((uint32_t)0x000000C0)

Trim retry count limitation is 512

Definition at line 88 of file sys.h.

## ◆ SYS_IRCTRIMCTL_RETRY_64

#define SYS_IRCTRIMCTL_RETRY_64 ((uint32_t)0x00000000)

Trim retry count limitation is 64

Definition at line 85 of file sys.h.

## ◆ SYS_IRCTRIMCTL_TRIM_11_0592M

#define SYS_IRCTRIMCTL_TRIM_11_0592M ((uint32_t)0x00000001)

Trim HIRC to 11.0592 MHz

Definition at line 76 of file sys.h.

## ◆ SYS_IRCTRIMCTL_TRIM_12M

#define SYS_IRCTRIMCTL_TRIM_12M ((uint32_t)0x00000002)

Trim HIRC to 12 MHz

Definition at line 77 of file sys.h.

## ◆ SYS_IRCTRIMCTL_TRIM_16M

#define SYS_IRCTRIMCTL_TRIM_16M ((uint32_t)0x00000003)

Trim HIRC to 16 MHz

Definition at line 78 of file sys.h.

## ◆ SYS_IRCTRIMIEN_32KERR_EN

#define SYS_IRCTRIMIEN_32KERR_EN ((uint32_t)0x00000004)

32.768 kHz Clock Error Interrupt Enable

Definition at line 95 of file sys.h.

## ◆ SYS_IRCTRIMIEN_DISABLE

#define SYS_IRCTRIMIEN_DISABLE ((uint32_t)0x00000000)

Trim failure interrupt disable

Definition at line 93 of file sys.h.

## ◆ SYS_IRCTRIMIEN_FAIL_EN

#define SYS_IRCTRIMIEN_FAIL_EN ((uint32_t)0x00000002)

Trim failure interrupt enable

Definition at line 94 of file sys.h.

## ◆ SYS_IRCTRIMINT_32KERR_INT

#define SYS_IRCTRIMINT_32KERR_INT ((uint32_t)0x00000004)

32.768 kHz Clock Error Interrupt Status

Definition at line 100 of file sys.h.

## ◆ SYS_IRCTRIMINT_FAIL_INT

#define SYS_IRCTRIMINT_FAIL_INT ((uint32_t)0x00000002)

Trim failure interrupt status

Definition at line 99 of file sys.h.

## ◆ SYS_IRCTRIMINT_FREQLOCK

#define SYS_IRCTRIMINT_FREQLOCK ((uint32_t)0x00000001)

HIRC frequency lock status

Definition at line 98 of file sys.h.

## ◆ SYS_LDOCTL_LDO_LEVEL16

#define SYS_LDOCTL_LDO_LEVEL16 ((uint32_t)0x00000004)

LDO Output 1.6 Voltage

Definition at line 71 of file sys.h.

## ◆ SYS_LDOCTL_LDO_LEVEL18

#define SYS_LDOCTL_LDO_LEVEL18 ((uint32_t)0x00000008)

LDO Output 1.8 Voltage

Definition at line 72 of file sys.h.

## ◆ SYS_LDOCTL_LDO_PD

#define SYS_LDOCTL_LDO_PD ((uint32_t)0x00000001)

LDO Disabled

Definition at line 70 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_GPA10

#define SYS_PA_H_MFP_PA10_MFP_GPA10 (0UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - GPIOA[10]

Definition at line 185 of file sys.h.

## ◆ SYS_PA_H_MFP_PA10_MFP_SC0_CLK

#define SYS_PA_H_MFP_PA10_MFP_SC0_CLK (4UL<<SYS_PA_H_MFP_PA10_MFP_Pos)

PA10 Pin Function - SmartCard0 clock

Definition at line 186 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_ADC_EXT

#define SYS_PA_H_MFP_PA11_MFP_ADC_EXT (2UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - ADC external trigger

Definition at line 182 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_GPA11

#define SYS_PA_H_MFP_PA11_MFP_GPA11 (0UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - GPIOA[11]

Definition at line 181 of file sys.h.

## ◆ SYS_PA_H_MFP_PA11_MFP_SC0_DAT

#define SYS_PA_H_MFP_PA11_MFP_SC0_DAT (4UL<<SYS_PA_H_MFP_PA11_MFP_Pos)

PA11 Pin Function - SmartCard0 DATA

Definition at line 183 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_ACMP1_P

#define SYS_PA_H_MFP_PA12_MFP_ACMP1_P (3UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - Comparator1 N-end input

Definition at line 175 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_GPA12

#define SYS_PA_H_MFP_PA12_MFP_GPA12 (0UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - GPIOA[12]

Definition at line 174 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_I2C0_SCL

#define SYS_PA_H_MFP_PA12_MFP_I2C0_SCL (5UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - I2C0 clock pin

Definition at line 176 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_LCD_S19

#define SYS_PA_H_MFP_PA12_MFP_LCD_S19 (8UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - LCD SEG 19

Definition at line 179 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_SPI1_MOSI0

#define SYS_PA_H_MFP_PA12_MFP_SPI1_MOSI0 (6UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - SPI1 MOSI[0]

Definition at line 177 of file sys.h.

## ◆ SYS_PA_H_MFP_PA12_MFP_UART0_TX

#define SYS_PA_H_MFP_PA12_MFP_UART0_TX (7UL<<SYS_PA_H_MFP_PA12_MFP_Pos)

PA12 Pin Function - UART1 TX

Definition at line 178 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_ACMP1_N

#define SYS_PA_H_MFP_PA13_MFP_ACMP1_N (3UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - Comparator1 N-end input

Definition at line 168 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_GPA13

#define SYS_PA_H_MFP_PA13_MFP_GPA13 (0UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - GPIOA[13]

Definition at line 167 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_I2C0_SDA

#define SYS_PA_H_MFP_PA13_MFP_I2C0_SDA (5UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - I2C0 data I/O pin

Definition at line 169 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_LCD_S18

#define SYS_PA_H_MFP_PA13_MFP_LCD_S18 (8UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - LCD SEG 18

Definition at line 172 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_SPI1_MISO0

#define SYS_PA_H_MFP_PA13_MFP_SPI1_MISO0 (6UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - SPI1 MISO[0]

Definition at line 170 of file sys.h.

## ◆ SYS_PA_H_MFP_PA13_MFP_UART0_RX

#define SYS_PA_H_MFP_PA13_MFP_UART0_RX (7UL<<SYS_PA_H_MFP_PA13_MFP_Pos)

PA13 Pin Function - UART1 RX

Definition at line 171 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_ACMP0_C

#define SYS_PA_H_MFP_PA14_MFP_ACMP0_C (9UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - Comparator0 charge/discharge path

Definition at line 165 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_GPA14

#define SYS_PA_H_MFP_PA14_MFP_GPA14 (0UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - GPIOA[14]

Definition at line 160 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_I2C1_SCL

#define SYS_PA_H_MFP_PA14_MFP_I2C1_SCL (5UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - I2C1 clock pin

Definition at line 161 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_LCD_S17

#define SYS_PA_H_MFP_PA14_MFP_LCD_S17 (8UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - LCD SEG 17

Definition at line 163 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_LCD_S31

#define SYS_PA_H_MFP_PA14_MFP_LCD_S31 (8UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - LCD SEG 31

Definition at line 164 of file sys.h.

## ◆ SYS_PA_H_MFP_PA14_MFP_SPI1_SCLK

#define SYS_PA_H_MFP_PA14_MFP_SPI1_SCLK (6UL<<SYS_PA_H_MFP_PA14_MFP_Pos)

PA14 Pin Function - SPI1 clock pin

Definition at line 162 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_ACMP1_O

#define SYS_PA_H_MFP_PA15_MFP_ACMP1_O (3UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - Comparator1 output

Definition at line 154 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_GPA15

#define SYS_PA_H_MFP_PA15_MFP_GPA15 (0UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - GPIOA[15]

Definition at line 152 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_I2C1_SDA

#define SYS_PA_H_MFP_PA15_MFP_I2C1_SDA (5UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - I2C1 data I/O pin

Definition at line 155 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_LCD_S16

#define SYS_PA_H_MFP_PA15_MFP_LCD_S16 (8UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - LCD SEG 16

Definition at line 157 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_LCD_S30

#define SYS_PA_H_MFP_PA15_MFP_LCD_S30 (8UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - LCD SEG 30

Definition at line 158 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_SPI1_SS0

#define SYS_PA_H_MFP_PA15_MFP_SPI1_SS0 (6UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - SPI1 1st chip selection

Definition at line 156 of file sys.h.

## ◆ SYS_PA_H_MFP_PA15_MFP_TMR3_CAP

#define SYS_PA_H_MFP_PA15_MFP_TMR3_CAP (2UL<<SYS_PA_H_MFP_PA15_MFP_Pos)

PA15 Pin Function - Timer1 capture event

Definition at line 153 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_GPA8

#define SYS_PA_H_MFP_PA8_MFP_GPA8 (0UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - GPIOA[8]

Definition at line 191 of file sys.h.

## ◆ SYS_PA_H_MFP_PA8_MFP_SC0_PWR

#define SYS_PA_H_MFP_PA8_MFP_SC0_PWR (4UL<<SYS_PA_H_MFP_PA8_MFP_Pos)

PA8 Pin Function - SmartCard0 power

Definition at line 192 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_GPA9

#define SYS_PA_H_MFP_PA9_MFP_GPA9 (0UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - GPIOA[9]

Definition at line 188 of file sys.h.

## ◆ SYS_PA_H_MFP_PA9_MFP_SC0_RST

#define SYS_PA_H_MFP_PA9_MFP_SC0_RST (4UL<<SYS_PA_H_MFP_PA9_MFP_Pos)

PA9 Pin Function - SmartCard0 RST

Definition at line 189 of file sys.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_ADC_CH0

#define SYS_PA_L_MFP_PA0_MFP_ADC_CH0 (2UL<<SYS_PA_L_MFP_PA0_MFP_Pos)

PA0 Pin Function - ADC input channel 0

Definition at line 149 of file sys.h.

## ◆ SYS_PA_L_MFP_PA0_MFP_GPA0

#define SYS_PA_L_MFP_PA0_MFP_GPA0 (0UL<<SYS_PA_L_MFP_PA0_MFP_Pos)

PA0 Pin Function - GPIOA[0]

Definition at line 148 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_ACMP0_C

#define SYS_PA_L_MFP_PA1_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - Comparator0 charge/discharge path

Definition at line 146 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_ACMP0_P

#define SYS_PA_L_MFP_PA1_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - Comparator0 P-end input3

Definition at line 145 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_ADC_CH1

#define SYS_PA_L_MFP_PA1_MFP_ADC_CH1 (2UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - ADC input channel 1

Definition at line 144 of file sys.h.

## ◆ SYS_PA_L_MFP_PA1_MFP_GPA1

#define SYS_PA_L_MFP_PA1_MFP_GPA1 (0UL<<SYS_PA_L_MFP_PA1_MFP_Pos)

PA1 Pin Function - GPIOA[1]

Definition at line 143 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_ACMP0_C

#define SYS_PA_L_MFP_PA2_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - Comparator0 charge/discharge path

Definition at line 141 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_ACMP0_P

#define SYS_PA_L_MFP_PA2_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - Comparator0 P-end input3

Definition at line 139 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_ADC_CH2

#define SYS_PA_L_MFP_PA2_MFP_ADC_CH2 (2UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - ADC input channel 2

Definition at line 138 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_EINT0

#define SYS_PA_L_MFP_PA2_MFP_EINT0 (1UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - External interrupt 0

Definition at line 137 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_GPA2

#define SYS_PA_L_MFP_PA2_MFP_GPA2 (0UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - GPIOA[2]

Definition at line 136 of file sys.h.

## ◆ SYS_PA_L_MFP_PA2_MFP_SC0_CLK

#define SYS_PA_L_MFP_PA2_MFP_SC0_CLK (4UL<<SYS_PA_L_MFP_PA2_MFP_Pos)

PA2 Pin Function - SmartCard0 clock

Definition at line 140 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_ACMP0_C

#define SYS_PA_L_MFP_PA3_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - Comparator0 charge/discharge path

Definition at line 134 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_ACMP0_P

#define SYS_PA_L_MFP_PA3_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - Comparator0 P-end input1

Definition at line 132 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_ADC_CH3

#define SYS_PA_L_MFP_PA3_MFP_ADC_CH3 (2UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - ADC input channel 3

Definition at line 131 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_EINT1

#define SYS_PA_L_MFP_PA3_MFP_EINT1 (1UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - External interrupt 1

Definition at line 130 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_GPA3

#define SYS_PA_L_MFP_PA3_MFP_GPA3 (0UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - GPIOA[3]

Definition at line 129 of file sys.h.

## ◆ SYS_PA_L_MFP_PA3_MFP_SC0_DAT

#define SYS_PA_L_MFP_PA3_MFP_SC0_DAT (4UL<<SYS_PA_L_MFP_PA3_MFP_Pos)

PA3 Pin Function - SmartCard0 DATA

Definition at line 133 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_ACMP0_C

#define SYS_PA_L_MFP_PA4_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - Comparator0 charge/discharge path

Definition at line 127 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_ACMP0_P

#define SYS_PA_L_MFP_PA4_MFP_ACMP0_P (3UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - Comparator0 P-end input0

Definition at line 125 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_ADC_CH4

#define SYS_PA_L_MFP_PA4_MFP_ADC_CH4 (2UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - ADC input channel 4

Definition at line 124 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_GPA4

#define SYS_PA_L_MFP_PA4_MFP_GPA4 (0UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - GPIOA[4]

Definition at line 123 of file sys.h.

## ◆ SYS_PA_L_MFP_PA4_MFP_SC0_CD

#define SYS_PA_L_MFP_PA4_MFP_SC0_CD (4UL<<SYS_PA_L_MFP_PA4_MFP_Pos)

PA4 Pin Function - SmartCard0 card detect pin

Definition at line 126 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_ACMP0_C

#define SYS_PA_L_MFP_PA5_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - Comparator0 charge/discharge path

Definition at line 121 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_ACMP0_N

#define SYS_PA_L_MFP_PA5_MFP_ACMP0_N (3UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - Comparator0 N-end input0

Definition at line 117 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_ADC_CH5

#define SYS_PA_L_MFP_PA5_MFP_ADC_CH5 (2UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - ADC input channel 5

Definition at line 116 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_GPA5

#define SYS_PA_L_MFP_PA5_MFP_GPA5 (0UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - GPIOA[5]

Definition at line 115 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_I2C1_SDA

#define SYS_PA_L_MFP_PA5_MFP_I2C1_SDA (5UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - I2C1 data I/O pin

Definition at line 119 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_SC0_PWR

#define SYS_PA_L_MFP_PA5_MFP_SC0_PWR (4UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - SmartCard0 Power pin

Definition at line 118 of file sys.h.

## ◆ SYS_PA_L_MFP_PA5_MFP_SPI1_SS0

#define SYS_PA_L_MFP_PA5_MFP_SPI1_SS0 (6UL<<SYS_PA_L_MFP_PA5_MFP_Pos)

PA5 Pin Function - SPI1 1st chip selection

Definition at line 120 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_ACMP0_C

#define SYS_PA_L_MFP_PA6_MFP_ACMP0_C (9UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - Comparator0 charge/discharge path

Definition at line 112 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_ACMP0_O

#define SYS_PA_L_MFP_PA6_MFP_ACMP0_O (3UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - Comparator0 output

Definition at line 110 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_ADC_CH6

#define SYS_PA_L_MFP_PA6_MFP_ADC_CH6 (2UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - ADC input channel 6

Definition at line 109 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_GPA6

#define SYS_PA_L_MFP_PA6_MFP_GPA6 (0UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - GPIOA[6]

Definition at line 108 of file sys.h.

## ◆ SYS_PA_L_MFP_PA6_MFP_SC0_RST

#define SYS_PA_L_MFP_PA6_MFP_SC0_RST (4UL<<SYS_PA_L_MFP_PA6_MFP_Pos)

PA6 Pin Function - SmartCard0 RST pin

Definition at line 111 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_ADC_CH7

#define SYS_PA_L_MFP_PA7_MFP_ADC_CH7 (2UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - ADC input channel 7

Definition at line 104 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_GPA7

#define SYS_PA_L_MFP_PA7_MFP_GPA7 (0UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - GPIOA[7]

Definition at line 103 of file sys.h.

## ◆ SYS_PA_L_MFP_PA7_MFP_SC1_CD

#define SYS_PA_L_MFP_PA7_MFP_SC1_CD (4UL<<SYS_PA_L_MFP_PA7_MFP_Pos)

PA7 Pin Function - SmartCard 1 detect pin

Definition at line 105 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_GPB10

#define SYS_PB_H_MFP_PB10_MFP_GPB10 (0UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - GPIOB[10]

Definition at line 283 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_LCD_S24

#define SYS_PB_H_MFP_PB10_MFP_LCD_S24 (8UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - LCD SEG 24

Definition at line 286 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_LCD_S28

#define SYS_PB_H_MFP_PB10_MFP_LCD_S28 (8UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - LCD SEG 28

Definition at line 287 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI1

#define SYS_PB_H_MFP_PB10_MFP_SPI0_MOSI1 (6UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - SPI0 MOSI[1]

Definition at line 284 of file sys.h.

## ◆ SYS_PB_H_MFP_PB10_MFP_UART1_RX

#define SYS_PB_H_MFP_PB10_MFP_UART1_RX (7UL<<SYS_PB_H_MFP_PB10_MFP_Pos)

PB10 Pin Function - UART1 RX

Definition at line 285 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_GPB11

#define SYS_PB_H_MFP_PB11_MFP_GPB11 (0UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - GPIOB[11]

Definition at line 275 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_LCD_S23

#define SYS_PB_H_MFP_PB11_MFP_LCD_S23 (8UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - LCD SEG 23

Definition at line 279 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_LCD_S27

#define SYS_PB_H_MFP_PB11_MFP_LCD_S27 (8UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - LCD SEG 27

Definition at line 280 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_SPI0_MISO1

#define SYS_PB_H_MFP_PB11_MFP_SPI0_MISO1 (6UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - SPI0 MISO[1]

Definition at line 277 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_TMR1_CNT

#define SYS_PB_H_MFP_PB11_MFP_TMR1_CNT (2UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - Timer1 external event input

Definition at line 276 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_TMR1_OUT

#define SYS_PB_H_MFP_PB11_MFP_TMR1_OUT (0xAUL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - Timer1 toggle out

Definition at line 281 of file sys.h.

## ◆ SYS_PB_H_MFP_PB11_MFP_UART1_RTS

#define SYS_PB_H_MFP_PB11_MFP_UART1_RTS (7UL<<SYS_PB_H_MFP_PB11_MFP_Pos)

PB11 Pin Function - UART1 RTSn

Definition at line 278 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_CKO0

#define SYS_PB_H_MFP_PB12_MFP_CKO0 (1UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - Frequency Divider0 output pin

Definition at line 266 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_GPB12

#define SYS_PB_H_MFP_PB12_MFP_GPB12 (0UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - GPIOB[12]

Definition at line 265 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_LCD_S15

#define SYS_PB_H_MFP_PB12_MFP_LCD_S15 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - LCD SEG 15

Definition at line 270 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_LCD_S22

#define SYS_PB_H_MFP_PB12_MFP_LCD_S22 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - LCD SEG 22

Definition at line 271 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_LCD_S26

#define SYS_PB_H_MFP_PB12_MFP_LCD_S26 (8UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - LCD SEG 26

Definition at line 272 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_SPI0_MOSI0

#define SYS_PB_H_MFP_PB12_MFP_SPI0_MOSI0 (6UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - SPI0 MOSI[0]

Definition at line 268 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_TMR0_CNT

#define SYS_PB_H_MFP_PB12_MFP_TMR0_CNT (2UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - Timer0 external counter input

Definition at line 267 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_TMR0_OUT

#define SYS_PB_H_MFP_PB12_MFP_TMR0_OUT (0xAUL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - Timer0 toggle out

Definition at line 273 of file sys.h.

## ◆ SYS_PB_H_MFP_PB12_MFP_UART0_RTS

#define SYS_PB_H_MFP_PB12_MFP_UART0_RTS (7UL<<SYS_PB_H_MFP_PB12_MFP_Pos)

PB12 Pin Function - UART0 RTSn

Definition at line 269 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_GPB13

#define SYS_PB_H_MFP_PB13_MFP_GPB13 (0UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - GPIOB[13]

Definition at line 258 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_LCD_S14

#define SYS_PB_H_MFP_PB13_MFP_LCD_S14 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - LCD SEG 14

Definition at line 261 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_LCD_S21

#define SYS_PB_H_MFP_PB13_MFP_LCD_S21 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - LCD SEG 21

Definition at line 262 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_LCD_S25

#define SYS_PB_H_MFP_PB13_MFP_LCD_S25 (8UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - LCD SEG 25

Definition at line 263 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_SPI0_MISO0

#define SYS_PB_H_MFP_PB13_MFP_SPI0_MISO0 (6UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - SPI0 MISO[0]

Definition at line 259 of file sys.h.

## ◆ SYS_PB_H_MFP_PB13_MFP_UART0_RX

#define SYS_PB_H_MFP_PB13_MFP_UART0_RX (7UL<<SYS_PB_H_MFP_PB13_MFP_Pos)

PB13 Pin Function - UART0 RX

Definition at line 260 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_GPB14

#define SYS_PB_H_MFP_PB14_MFP_GPB14 (0UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - GPIOB[14]

Definition at line 251 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_LCD_S13

#define SYS_PB_H_MFP_PB14_MFP_LCD_S13 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - LCD SEG 13

Definition at line 254 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_LCD_S20

#define SYS_PB_H_MFP_PB14_MFP_LCD_S20 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - LCD SEG 20

Definition at line 255 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_LCD_S24

#define SYS_PB_H_MFP_PB14_MFP_LCD_S24 (8UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB14 Pin Function - LCD SEG 24

Definition at line 256 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_SPI0_SCLK

#define SYS_PB_H_MFP_PB14_MFP_SPI0_SCLK (6UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB15 Pin Function - SPI0 serial clock pin

Definition at line 252 of file sys.h.

## ◆ SYS_PB_H_MFP_PB14_MFP_UART0_TX

#define SYS_PB_H_MFP_PB14_MFP_UART0_TX (7UL<<SYS_PB_H_MFP_PB14_MFP_Pos)

PB15 Pin Function - UART0 TX

Definition at line 253 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_GPB15

#define SYS_PB_H_MFP_PB15_MFP_GPB15 (0UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - GPIOB[15]

Definition at line 244 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_LCD_S12

#define SYS_PB_H_MFP_PB15_MFP_LCD_S12 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - LCD SEG 12

Definition at line 247 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_LCD_S19

#define SYS_PB_H_MFP_PB15_MFP_LCD_S19 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - LCD SEG 19

Definition at line 248 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_LCD_S23

#define SYS_PB_H_MFP_PB15_MFP_LCD_S23 (8UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - LCD SEG 23

Definition at line 249 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_SPI0_SS0

#define SYS_PB_H_MFP_PB15_MFP_SPI0_SS0 (6UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - SPI0 1st slave select pin

Definition at line 245 of file sys.h.

## ◆ SYS_PB_H_MFP_PB15_MFP_UART0_CTS

#define SYS_PB_H_MFP_PB15_MFP_UART0_CTS (7UL<<SYS_PB_H_MFP_PB15_MFP_Pos)

PB15 Pin Function - UART0 CTSn

Definition at line 246 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_EINT1

#define SYS_PB_H_MFP_PB8_MFP_EINT1 (1UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - External interrupt1 input pin

Definition at line 294 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_GPB8

#define SYS_PB_H_MFP_PB8_MFP_GPB8 (0UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - GPIOB[8]

Definition at line 293 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_LCD_S32

#define SYS_PB_H_MFP_PB8_MFP_LCD_S32 (8UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - LCD SEG 32

Definition at line 298 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_PWM0_CH0

#define SYS_PB_H_MFP_PB8_MFP_PWM0_CH0 (3UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - PWM0 Channel0 output

Definition at line 296 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_SNOOPER

#define SYS_PB_H_MFP_PB8_MFP_SNOOPER (4UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - Snooper pin

Definition at line 297 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_TMR0_CNT

#define SYS_PB_H_MFP_PB8_MFP_TMR0_CNT (2UL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - Timer0 external counter input

Definition at line 295 of file sys.h.

## ◆ SYS_PB_H_MFP_PB8_MFP_TMR0_OUT

#define SYS_PB_H_MFP_PB8_MFP_TMR0_OUT (0xAUL<<SYS_PB_H_MFP_PB8_MFP_Pos)

PB8 Pin Function - Timer0 toggle out

Definition at line 299 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_GPB9

#define SYS_PB_H_MFP_PB9_MFP_GPB9 (0UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - GPIOB[9]

Definition at line 289 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_LCD_S31

#define SYS_PB_H_MFP_PB9_MFP_LCD_S31 (8UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - LCD SEG 31

Definition at line 291 of file sys.h.

## ◆ SYS_PB_H_MFP_PB9_MFP_PWM0_CH1

#define SYS_PB_H_MFP_PB9_MFP_PWM0_CH1 (3UL<<SYS_PB_H_MFP_PB9_MFP_Pos)

PB9 Pin Function - PWM0 Channel1 output

Definition at line 290 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_CKO1

#define SYS_PB_L_MFP_PB0_MFP_CKO1 (1UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - Frequency Divider1 output pin

Definition at line 239 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_GPB0

#define SYS_PB_L_MFP_PB0_MFP_GPB0 (0UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - GPIOB[0]

Definition at line 238 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_LCD_S29

#define SYS_PB_L_MFP_PB0_MFP_LCD_S29 (8UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - LCD SEG 29

Definition at line 241 of file sys.h.

## ◆ SYS_PB_L_MFP_PB0_MFP_UART0_TX

#define SYS_PB_L_MFP_PB0_MFP_UART0_TX (7UL<<SYS_PB_L_MFP_PB0_MFP_Pos)

PB0 Pin Function - UART0 TX

Definition at line 240 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_EINT1

#define SYS_PB_L_MFP_PB1_MFP_EINT1 (1UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - External interrupt1 input pin

Definition at line 233 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_GPB1

#define SYS_PB_L_MFP_PB1_MFP_GPB1 (0UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - GPIOB[1]

Definition at line 232 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_LCD_S28

#define SYS_PB_L_MFP_PB1_MFP_LCD_S28 (8UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - LCD SEG 28

Definition at line 236 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_TMR2_CAP

#define SYS_PB_L_MFP_PB1_MFP_TMR2_CAP (2UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - Timer2 capture event

Definition at line 234 of file sys.h.

## ◆ SYS_PB_L_MFP_PB1_MFP_UART0_RX

#define SYS_PB_L_MFP_PB1_MFP_UART0_RX (7UL<<SYS_PB_L_MFP_PB1_MFP_Pos)

PB1 Pin Function - UART0 RX

Definition at line 235 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_GPB2

#define SYS_PB_L_MFP_PB2_MFP_GPB2 (0UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - GPIOB[2]

Definition at line 224 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_I2C0_SCL

#define SYS_PB_L_MFP_PB2_MFP_I2C0_SCL (5UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - I2C0 clock pin

Definition at line 226 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_LCD_S27

#define SYS_PB_L_MFP_PB2_MFP_LCD_S27 (8UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - LCD SEG 27

Definition at line 229 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_SPI1_MOSI1

#define SYS_PB_L_MFP_PB2_MFP_SPI1_MOSI1 (6UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - SPI1 MOSI[1]

Definition at line 227 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_TMR3_CNT

#define SYS_PB_L_MFP_PB2_MFP_TMR3_CNT (2UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - Timer3 external counter input

Definition at line 225 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_TMR3_OUT

#define SYS_PB_L_MFP_PB2_MFP_TMR3_OUT (0xAUL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - Timer3 toggle out

Definition at line 230 of file sys.h.

## ◆ SYS_PB_L_MFP_PB2_MFP_UART0_RTS

#define SYS_PB_L_MFP_PB2_MFP_UART0_RTS (7UL<<SYS_PB_L_MFP_PB2_MFP_Pos)

PB2 Pin Function - UART0 RTSn

Definition at line 228 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_GPB3

#define SYS_PB_L_MFP_PB3_MFP_GPB3 (0UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - GPIOB[3]

Definition at line 216 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_I2C0_SDA

#define SYS_PB_L_MFP_PB3_MFP_I2C0_SDA (5UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - I2C0 data I/O pin

Definition at line 218 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_LCD_S26

#define SYS_PB_L_MFP_PB3_MFP_LCD_S26 (8UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - LCD SEG 26

Definition at line 221 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_SPI1_MISO1

#define SYS_PB_L_MFP_PB3_MFP_SPI1_MISO1 (6UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - SPI1 MISO[1]

Definition at line 219 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_TMR2_CNT

#define SYS_PB_L_MFP_PB3_MFP_TMR2_CNT (2UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - Timer2 external counter input

Definition at line 217 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_TMR2_OUT

#define SYS_PB_L_MFP_PB3_MFP_TMR2_OUT (0xAUL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - Timer2 toggle out

Definition at line 222 of file sys.h.

## ◆ SYS_PB_L_MFP_PB3_MFP_UART0_CTS

#define SYS_PB_L_MFP_PB3_MFP_UART0_CTS (7UL<<SYS_PB_L_MFP_PB3_MFP_Pos)

PB3 Pin Function - UART0 CTSn

Definition at line 220 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_GPB4

#define SYS_PB_L_MFP_PB4_MFP_GPB4 (0UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - GPIOB[4]

Definition at line 212 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_SPI1_MISO1

#define SYS_PB_L_MFP_PB4_MFP_SPI1_MISO1 (6UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - SPI2 MISO[1]

Definition at line 213 of file sys.h.

## ◆ SYS_PB_L_MFP_PB4_MFP_UART1_RTS

#define SYS_PB_L_MFP_PB4_MFP_UART1_RTS (7UL<<SYS_PB_L_MFP_PB4_MFP_Pos)

PB4 Pin Function - UART1 RTS

Definition at line 214 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_GPB5

#define SYS_PB_L_MFP_PB5_MFP_GPB5 (0UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - GPIOB[5]

Definition at line 207 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_LCD_S35

#define SYS_PB_L_MFP_PB5_MFP_LCD_S35 (8UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - LCD SEG 35

Definition at line 210 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_SPI1_MOSI1

#define SYS_PB_L_MFP_PB5_MFP_SPI1_MOSI1 (6UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - SPI1 MOSI[1]

Definition at line 208 of file sys.h.

## ◆ SYS_PB_L_MFP_PB5_MFP_UART1_RX

#define SYS_PB_L_MFP_PB5_MFP_UART1_RX (7UL<<SYS_PB_L_MFP_PB5_MFP_Pos)

PB5 Pin Function - UART1 RX

Definition at line 209 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_CKO0

#define SYS_PB_L_MFP_PB6_MFP_CKO0 (1UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - Frequency Divider0 output pin

Definition at line 201 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_GPB6

#define SYS_PB_L_MFP_PB6_MFP_GPB6 (0UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - GPIOB[6]

Definition at line 200 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_LCD_S25

#define SYS_PB_L_MFP_PB6_MFP_LCD_S25 (8UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - LCD SEG 25

Definition at line 204 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_LCD_S34

#define SYS_PB_L_MFP_PB6_MFP_LCD_S34 (8UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - LCD SEG 34

Definition at line 205 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_SPI1_SS1

#define SYS_PB_L_MFP_PB6_MFP_SPI1_SS1 (6UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - SPI2 2nd slave select pin

Definition at line 202 of file sys.h.

## ◆ SYS_PB_L_MFP_PB6_MFP_UART1_TX

#define SYS_PB_L_MFP_PB6_MFP_UART1_TX (7UL<<SYS_PB_L_MFP_PB6_MFP_Pos)

PB6 Pin Function - UART1 TX

Definition at line 203 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_GPB7

#define SYS_PB_L_MFP_PB7_MFP_GPB7 (0UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - GPIOB[7]

Definition at line 195 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_LCD_S33

#define SYS_PB_L_MFP_PB7_MFP_LCD_S33 (8UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - LCD SEG 33

Definition at line 198 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_SC0_CD

#define SYS_PB_L_MFP_PB7_MFP_SC0_CD (4UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - SmartCard0 card detect

Definition at line 196 of file sys.h.

## ◆ SYS_PB_L_MFP_PB7_MFP_UART1_CTS

#define SYS_PB_L_MFP_PB7_MFP_UART1_CTS (7UL<<SYS_PB_L_MFP_PB7_MFP_Pos)

PB7 Pin Function - UART1 CTSn

Definition at line 197 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_GPC10

#define SYS_PC_H_MFP_PC10_MFP_GPC10 (0UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - GPIOC[10]

Definition at line 383 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_I2C1_SCL

#define SYS_PC_H_MFP_PC10_MFP_I2C1_SCL (5UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - I2C1 clock pin

Definition at line 385 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_LCD_S12

#define SYS_PC_H_MFP_PC10_MFP_LCD_S12 (8UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - LCD SEG 12

Definition at line 386 of file sys.h.

## ◆ SYS_PC_H_MFP_PC10_MFP_SC1_CD

#define SYS_PC_H_MFP_PC10_MFP_SC1_CD (4UL<<SYS_PC_H_MFP_PC10_MFP_Pos)

PC10 Pin Function - SmartCard1 card detect

Definition at line 384 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_GPC11

#define SYS_PC_H_MFP_PC11_MFP_GPC11 (0UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - GPIOC[11]

Definition at line 378 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_I2C1_SDA

#define SYS_PC_H_MFP_PC11_MFP_I2C1_SDA (5UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - I2C1 data I/O pin

Definition at line 380 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_LCD_S11

#define SYS_PC_H_MFP_PC11_MFP_LCD_S11 (8UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - LCD SEG 11

Definition at line 381 of file sys.h.

## ◆ SYS_PC_H_MFP_PC11_MFP_SC1_PWR

#define SYS_PC_H_MFP_PC11_MFP_SC1_PWR (4UL<<SYS_PC_H_MFP_PC11_MFP_Pos)

PC11 Pin Function - SmartCard1 PWR pin

Definition at line 379 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_GPC12

#define SYS_PC_H_MFP_PC12_MFP_GPC12 (0UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - GPIOC[12]

Definition at line 374 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_LCD_S10

#define SYS_PC_H_MFP_PC12_MFP_LCD_S10 (8UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - LCD SEG 10

Definition at line 376 of file sys.h.

## ◆ SYS_PC_H_MFP_PC12_MFP_SC1_CLK

#define SYS_PC_H_MFP_PC12_MFP_SC1_CLK (4UL<<SYS_PC_H_MFP_PC12_MFP_Pos)

PC12 Pin Function - SmartCard1 clock

Definition at line 375 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_GPC13

#define SYS_PC_H_MFP_PC13_MFP_GPC13 (0UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - GPIOC[13]

Definition at line 370 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_LCD_S9

#define SYS_PC_H_MFP_PC13_MFP_LCD_S9 (8UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - LCD SEG 9

Definition at line 372 of file sys.h.

## ◆ SYS_PC_H_MFP_PC13_MFP_SC1_DAT

#define SYS_PC_H_MFP_PC13_MFP_SC1_DAT (4UL<<SYS_PC_H_MFP_PC13_MFP_Pos)

PC13 Pin Function - SmartCard1 DATA

Definition at line 371 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_GPC14

#define SYS_PC_H_MFP_PC14_MFP_GPC14 (0UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - GPIOC[14]

Definition at line 365 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_LCD_S1

#define SYS_PC_H_MFP_PC14_MFP_LCD_S1 (7UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - LCD SEG 1

Definition at line 367 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_LCD_S8

#define SYS_PC_H_MFP_PC14_MFP_LCD_S8 (8UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - LCD SEG 8

Definition at line 368 of file sys.h.

## ◆ SYS_PC_H_MFP_PC14_MFP_SC1_CD

#define SYS_PC_H_MFP_PC14_MFP_SC1_CD (4UL<<SYS_PC_H_MFP_PC14_MFP_Pos)

PC14 Pin Function - SmartCard1 card detect

Definition at line 366 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_GPC15

#define SYS_PC_H_MFP_PC15_MFP_GPC15 (0UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - GPIOC[15]

Definition at line 360 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_LCD_S0

#define SYS_PC_H_MFP_PC15_MFP_LCD_S0 (8UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - LCD SEG 0

Definition at line 362 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_LCD_S7

#define SYS_PC_H_MFP_PC15_MFP_LCD_S7 (8UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - LCD SEG 7

Definition at line 363 of file sys.h.

## ◆ SYS_PC_H_MFP_PC15_MFP_SC1_PWR

#define SYS_PC_H_MFP_PC15_MFP_SC1_PWR (4UL<<SYS_PC_H_MFP_PC15_MFP_Pos)

PC15 Pin Function - SmartCard1 PWR pin

Definition at line 361 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_GPC8

#define SYS_PC_H_MFP_PC8_MFP_GPC8 (0UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - GPIOC[8]

Definition at line 393 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_LCD_S10

#define SYS_PC_H_MFP_PC8_MFP_LCD_S10 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - LCD SEG 10

Definition at line 397 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_LCD_S14

#define SYS_PC_H_MFP_PC8_MFP_LCD_S14 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - LCD SEG 14

Definition at line 398 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_LCD_S3

#define SYS_PC_H_MFP_PC8_MFP_LCD_S3 (8UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - LCD SEG 3

Definition at line 396 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_SC0_RST

#define SYS_PC_H_MFP_PC8_MFP_SC0_RST (4UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - SmartCard0 RST pin

Definition at line 394 of file sys.h.

## ◆ SYS_PC_H_MFP_PC8_MFP_UART1_TX

#define SYS_PC_H_MFP_PC8_MFP_UART1_TX (7UL<<SYS_PC_H_MFP_PC8_MFP_Pos)

PC8 Pin Function - UART1 Data transmitter output pin

Definition at line 395 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_GPC9

#define SYS_PC_H_MFP_PC9_MFP_GPC9 (0UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - GPIOC[9]

Definition at line 388 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_LCD_S13

#define SYS_PC_H_MFP_PC9_MFP_LCD_S13 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - LCD SEG 13

Definition at line 391 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_LCD_S2

#define SYS_PC_H_MFP_PC9_MFP_LCD_S2 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - LCD SEG 2

Definition at line 389 of file sys.h.

## ◆ SYS_PC_H_MFP_PC9_MFP_LCD_S9

#define SYS_PC_H_MFP_PC9_MFP_LCD_S9 (8UL<<SYS_PC_H_MFP_PC9_MFP_Pos)

PC9 Pin Function - LCD SEG 9

Definition at line 390 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_GPC0

#define SYS_PC_L_MFP_PC0_MFP_GPC0 (0UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - GPIOC[0]

Definition at line 351 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_I2C0_SCL

#define SYS_PC_L_MFP_PC0_MFP_I2C0_SCL (5UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - I2C0 clock pin

Definition at line 353 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_LCD_S11

#define SYS_PC_L_MFP_PC0_MFP_LCD_S11 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - LCD SEG 11

Definition at line 355 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_LCD_S18

#define SYS_PC_L_MFP_PC0_MFP_LCD_S18 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - LCD SEG 18

Definition at line 356 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_LCD_S22

#define SYS_PC_L_MFP_PC0_MFP_LCD_S22 (8UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - LCD SEG 22

Definition at line 357 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_PWM0_CH0

#define SYS_PC_L_MFP_PC0_MFP_PWM0_CH0 (3UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - PWM0 Channel0 output

Definition at line 352 of file sys.h.

## ◆ SYS_PC_L_MFP_PC0_MFP_SPI0_SS1

#define SYS_PC_L_MFP_PC0_MFP_SPI0_SS1 (6UL<<SYS_PC_L_MFP_PC0_MFP_Pos)

PC0 Pin Function - SPI0 2nd slave select pin

Definition at line 354 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_GPC1

#define SYS_PC_L_MFP_PC1_MFP_GPC1 (0UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - GPIOC[1]

Definition at line 344 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_I2C0_SDA

#define SYS_PC_L_MFP_PC1_MFP_I2C0_SDA (5UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - I2C0 data I/O pin

Definition at line 346 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_LCD_S10

#define SYS_PC_L_MFP_PC1_MFP_LCD_S10 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - LCD SEG 10

Definition at line 347 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_LCD_S17

#define SYS_PC_L_MFP_PC1_MFP_LCD_S17 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - LCD SEG 17

Definition at line 348 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_LCD_S21

#define SYS_PC_L_MFP_PC1_MFP_LCD_S21 (8UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - LCD SEG 21

Definition at line 349 of file sys.h.

## ◆ SYS_PC_L_MFP_PC1_MFP_PWM0_CH1

#define SYS_PC_L_MFP_PC1_MFP_PWM0_CH1 (3UL<<SYS_PC_L_MFP_PC1_MFP_Pos)

PC1 Pin Function - PWM0 Channel1 output

Definition at line 345 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_GPC2

#define SYS_PC_L_MFP_PC2_MFP_GPC2 (0UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - GPIOC[2]

Definition at line 337 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_I2C1_SCL

#define SYS_PC_L_MFP_PC2_MFP_I2C1_SCL (5UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - I2C1 clock

Definition at line 339 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_LCD_S16

#define SYS_PC_L_MFP_PC2_MFP_LCD_S16 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - LCD SEG 16

Definition at line 341 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_LCD_S20

#define SYS_PC_L_MFP_PC2_MFP_LCD_S20 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - LCD SEG 20

Definition at line 342 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_LCD_S9

#define SYS_PC_L_MFP_PC2_MFP_LCD_S9 (8UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - LCD SEG 9

Definition at line 340 of file sys.h.

## ◆ SYS_PC_L_MFP_PC2_MFP_PWM0_CH2

#define SYS_PC_L_MFP_PC2_MFP_PWM0_CH2 (3UL<<SYS_PC_L_MFP_PC2_MFP_Pos)

PC2 Pin Function - PWM0 Channel2 output

Definition at line 338 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_GPC3

#define SYS_PC_L_MFP_PC3_MFP_GPC3 (0UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - GPIOC[3]

Definition at line 330 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_I2C1_SDA

#define SYS_PC_L_MFP_PC3_MFP_I2C1_SDA (5UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - I2C1 data I/O pin

Definition at line 332 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_LCD_S15

#define SYS_PC_L_MFP_PC3_MFP_LCD_S15 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - LCD SEG 15

Definition at line 334 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_LCD_S19

#define SYS_PC_L_MFP_PC3_MFP_LCD_S19 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - LCD SEG 19

Definition at line 335 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_LCD_S8

#define SYS_PC_L_MFP_PC3_MFP_LCD_S8 (8UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - LCD SEG 8

Definition at line 333 of file sys.h.

## ◆ SYS_PC_L_MFP_PC3_MFP_PWM0_CH3

#define SYS_PC_L_MFP_PC3_MFP_PWM0_CH3 (3UL<<SYS_PC_L_MFP_PC3_MFP_Pos)

PC3 Pin Function - PWM0 Channel3 output

Definition at line 331 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_EINT0

#define SYS_PC_L_MFP_PC4_MFP_EINT0 (1UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - External interrupt0 input pin

Definition at line 323 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_GPC4

#define SYS_PC_L_MFP_PC4_MFP_GPC4 (0UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - GPIOC[4]

Definition at line 322 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_LCD_S14

#define SYS_PC_L_MFP_PC4_MFP_LCD_S14 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - LCD SEG 14

Definition at line 327 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_LCD_S18

#define SYS_PC_L_MFP_PC4_MFP_LCD_S18 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - LCD SEG 18

Definition at line 328 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_LCD_S7

#define SYS_PC_L_MFP_PC4_MFP_LCD_S7 (8UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - LCD SEG 7

Definition at line 326 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_SC0_CLK

#define SYS_PC_L_MFP_PC4_MFP_SC0_CLK (4UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - SmartCard0 clock

Definition at line 324 of file sys.h.

## ◆ SYS_PC_L_MFP_PC4_MFP_UART1_CTS

#define SYS_PC_L_MFP_PC4_MFP_UART1_CTS (7UL<<SYS_PC_L_MFP_PC4_MFP_Pos)

PC4 Pin Function - UART1 CTSn

Definition at line 325 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_GPC5

#define SYS_PC_L_MFP_PC5_MFP_GPC5 (0UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - GPIOC[5]

Definition at line 316 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_LCD_S13

#define SYS_PC_L_MFP_PC5_MFP_LCD_S13 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - LCD SEG 13

Definition at line 319 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_LCD_S17

#define SYS_PC_L_MFP_PC5_MFP_LCD_S17 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - LCD SEG 17

Definition at line 320 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_LCD_S6

#define SYS_PC_L_MFP_PC5_MFP_LCD_S6 (8UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - LCD SEG 6

Definition at line 318 of file sys.h.

## ◆ SYS_PC_L_MFP_PC5_MFP_SC0_CD

#define SYS_PC_L_MFP_PC5_MFP_SC0_CD (4UL<<SYS_PC_L_MFP_PC5_MFP_Pos)

PC5 Pin Function - SmartCard0 card detect pin

Definition at line 317 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_GPC6

#define SYS_PC_L_MFP_PC6_MFP_GPC6 (0UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - GPIOC[6]

Definition at line 309 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_LCD_S12

#define SYS_PC_L_MFP_PC6_MFP_LCD_S12 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - LCD SEG 12

Definition at line 313 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_LCD_S16

#define SYS_PC_L_MFP_PC6_MFP_LCD_S16 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - LCD SEG 16

Definition at line 314 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_LCD_S5

#define SYS_PC_L_MFP_PC6_MFP_LCD_S5 (8UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - LCD SEG 5

Definition at line 312 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_SC0_DAT

#define SYS_PC_L_MFP_PC6_MFP_SC0_DAT (4UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - SmartCard0 data

Definition at line 310 of file sys.h.

## ◆ SYS_PC_L_MFP_PC6_MFP_UART1_RTS

#define SYS_PC_L_MFP_PC6_MFP_UART1_RTS (7UL<<SYS_PC_L_MFP_PC6_MFP_Pos)

PC6 Pin Function - UART1 RTSn

Definition at line 311 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_GPC7

#define SYS_PC_L_MFP_PC7_MFP_GPC7 (0UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - GPIOC[7]

Definition at line 302 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_LCD_S11

#define SYS_PC_L_MFP_PC7_MFP_LCD_S11 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - LCD SEG 11

Definition at line 306 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_LCD_S15

#define SYS_PC_L_MFP_PC7_MFP_LCD_S15 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - LCD SEG 15

Definition at line 307 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_LCD_S4

#define SYS_PC_L_MFP_PC7_MFP_LCD_S4 (8UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - LCD SEG 4

Definition at line 305 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_SC0_PWR

#define SYS_PC_L_MFP_PC7_MFP_SC0_PWR (4UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - SmartCard0 Power pin

Definition at line 303 of file sys.h.

## ◆ SYS_PC_L_MFP_PC7_MFP_UART1_RX

#define SYS_PC_L_MFP_PC7_MFP_UART1_RX (7UL<<SYS_PC_L_MFP_PC7_MFP_Pos)

PC7 Pin Function - UART1 RX

Definition at line 304 of file sys.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_GPD10

#define SYS_PD_H_MFP_PD10_MFP_GPD10 (0UL<<SYS_PD_H_MFP_PD10_MFP_Pos)

PD10 Pin Function - GPIOD[10]

Definition at line 453 of file sys.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_LCD_COM0

#define SYS_PD_H_MFP_PD10_MFP_LCD_COM0 (8UL<<SYS_PD_H_MFP_PD10_MFP_Pos)

PD10 Pin Function - LCD COM0

Definition at line 456 of file sys.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_PWM0_CH2

#define SYS_PD_H_MFP_PD10_MFP_PWM0_CH2 (3UL<<SYS_PD_H_MFP_PD10_MFP_Pos)

PD10 Pin Function - PWM0 Channel2 output

Definition at line 455 of file sys.h.

## ◆ SYS_PD_H_MFP_PD10_MFP_TMR1_CAP

#define SYS_PD_H_MFP_PD10_MFP_TMR1_CAP (2UL<<SYS_PD_H_MFP_PD10_MFP_Pos)

PD10 Pin Function - Timer1 capture input

Definition at line 454 of file sys.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_GPD11

#define SYS_PD_H_MFP_PD11_MFP_GPD11 (0UL<<SYS_PD_H_MFP_PD11_MFP_Pos)

PD11 Pin Function - GPIOD[11]

Definition at line 448 of file sys.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_LCD_DH2

#define SYS_PD_H_MFP_PD11_MFP_LCD_DH2 (8UL<<SYS_PD_H_MFP_PD11_MFP_Pos)

PD11 Pin Function - LCD DH2

Definition at line 451 of file sys.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_PWM0_CH1

#define SYS_PD_H_MFP_PD11_MFP_PWM0_CH1 (3UL<<SYS_PD_H_MFP_PD11_MFP_Pos)

PD11 Pin Function - PWM0 Channel1 output

Definition at line 450 of file sys.h.

## ◆ SYS_PD_H_MFP_PD11_MFP_TMR0_CAP

#define SYS_PD_H_MFP_PD11_MFP_TMR0_CAP (2UL<<SYS_PD_H_MFP_PD11_MFP_Pos)

PD11 Pin Function - Timer0 capture input

Definition at line 449 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_CKO0

#define SYS_PD_H_MFP_PD12_MFP_CKO0 (1UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - Frequency Divider0 output pin

Definition at line 441 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_CLK_Hz

#define SYS_PD_H_MFP_PD12_MFP_CLK_Hz (9UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - RTC output pin

Definition at line 445 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_GPD12

#define SYS_PD_H_MFP_PD12_MFP_GPD12 (0UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - GPIOD[12]

Definition at line 440 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_LCD_DH1

#define SYS_PD_H_MFP_PD12_MFP_LCD_DH1 (8UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - LCD DH1

Definition at line 444 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_PWM0_CH0

#define SYS_PD_H_MFP_PD12_MFP_PWM0_CH0 (3UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - PWM0 Channel0 output

Definition at line 443 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_TMR1_CNT

#define SYS_PD_H_MFP_PD12_MFP_TMR1_CNT (2UL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - Timer1 external counter input

Definition at line 442 of file sys.h.

## ◆ SYS_PD_H_MFP_PD12_MFP_TMR1_OUT

#define SYS_PD_H_MFP_PD12_MFP_TMR1_OUT (0xAUL<<SYS_PD_H_MFP_PD12_MFP_Pos)

PD12 Pin Function - Timer1 toggle out

Definition at line 446 of file sys.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_EINT1

#define SYS_PD_H_MFP_PD13_MFP_EINT1 (1UL<<SYS_PD_H_MFP_PD13_MFP_Pos)

PD13 Pin Function - External interrupt 1 input pin

Definition at line 437 of file sys.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_GPD13

#define SYS_PD_H_MFP_PD13_MFP_GPD13 (0UL<<SYS_PD_H_MFP_PD13_MFP_Pos)

PD13 Pin Function - GPIOD[13]

Definition at line 436 of file sys.h.

## ◆ SYS_PD_H_MFP_PD13_MFP_LCD_V1

#define SYS_PD_H_MFP_PD13_MFP_LCD_V1 (8UL<<SYS_PD_H_MFP_PD13_MFP_Pos)

PD13 Pin Function - LCD V1

Definition at line 438 of file sys.h.

## ◆ SYS_PD_H_MFP_PD14_MFP_GPD14

#define SYS_PD_H_MFP_PD14_MFP_GPD14 (0UL<<SYS_PD_H_MFP_PD14_MFP_Pos)

PD14 Pin Function - GPIOD[14]

Definition at line 433 of file sys.h.

## ◆ SYS_PD_H_MFP_PD14_MFP_LCD_V2

#define SYS_PD_H_MFP_PD14_MFP_LCD_V2 (8UL<<SYS_PD_H_MFP_PD14_MFP_Pos)

PD14 Pin Function - LCD V2

Definition at line 434 of file sys.h.

## ◆ SYS_PD_H_MFP_PD15_MFP_GPD15

#define SYS_PD_H_MFP_PD15_MFP_GPD15 (0UL<<SYS_PD_H_MFP_PD15_MFP_Pos)

PD15 Pin Function - GPIOD[15]

Definition at line 430 of file sys.h.

## ◆ SYS_PD_H_MFP_PD15_MFP_LCD_V3

#define SYS_PD_H_MFP_PD15_MFP_LCD_V3 (8UL<<SYS_PD_H_MFP_PD15_MFP_Pos)

PD15 Pin Function - LCD V3

Definition at line 431 of file sys.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_GPD8

#define SYS_PD_H_MFP_PD8_MFP_GPD8 (0UL<<SYS_PD_H_MFP_PD8_MFP_Pos)

PD8 Pin Function - GPIOD[8]

Definition at line 463 of file sys.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_LCD_COM2

#define SYS_PD_H_MFP_PD8_MFP_LCD_COM2 (8UL<<SYS_PD_H_MFP_PD8_MFP_Pos)

PD8 Pin Function - LCD COM2

Definition at line 465 of file sys.h.

## ◆ SYS_PD_H_MFP_PD8_MFP_SC1_DAT

#define SYS_PD_H_MFP_PD8_MFP_SC1_DAT (4UL<<SYS_PD_H_MFP_PD8_MFP_Pos)

PD8 Pin Function - SmartCard1 data

Definition at line 464 of file sys.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_GPD9

#define SYS_PD_H_MFP_PD9_MFP_GPD9 (0UL<<SYS_PD_H_MFP_PD9_MFP_Pos)

PD9 Pin Function - GPIOD[9]

Definition at line 458 of file sys.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_LCD_COM1

#define SYS_PD_H_MFP_PD9_MFP_LCD_COM1 (8UL<<SYS_PD_H_MFP_PD9_MFP_Pos)

PD9 Pin Function - LCD COM1

Definition at line 461 of file sys.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_PWM0_CH3

#define SYS_PD_H_MFP_PD9_MFP_PWM0_CH3 (3UL<<SYS_PD_H_MFP_PD9_MFP_Pos)

PD9 Pin Function - PWM0 Channel3 output

Definition at line 459 of file sys.h.

## ◆ SYS_PD_H_MFP_PD9_MFP_SC1_RST

#define SYS_PD_H_MFP_PD9_MFP_SC1_RST (4UL<<SYS_PD_H_MFP_PD9_MFP_Pos)

PD9 Pin Function - SmartCard1 RST pin

Definition at line 460 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_GPD0

#define SYS_PD_L_MFP_PD0_MFP_GPD0 (0UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - GPIOD[0]

Definition at line 426 of file sys.h.

## ◆ SYS_PD_L_MFP_PD0_MFP_LCD_S6

#define SYS_PD_L_MFP_PD0_MFP_LCD_S6 (8UL<<SYS_PD_L_MFP_PD0_MFP_Pos)

PD0 Pin Function - LCD SEG 6

Definition at line 427 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_GPD1

#define SYS_PD_L_MFP_PD1_MFP_GPD1 (0UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - GPIOD[1]

Definition at line 423 of file sys.h.

## ◆ SYS_PD_L_MFP_PD1_MFP_LCD_S5

#define SYS_PD_L_MFP_PD1_MFP_LCD_S5 (8UL<<SYS_PD_L_MFP_PD1_MFP_Pos)

PD1 Pin Function - LCD SEG 5

Definition at line 424 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_GPD2

#define SYS_PD_L_MFP_PD2_MFP_GPD2 (0UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - GPIOD[2]

Definition at line 420 of file sys.h.

## ◆ SYS_PD_L_MFP_PD2_MFP_LCD_S4

#define SYS_PD_L_MFP_PD2_MFP_LCD_S4 (8UL<<SYS_PD_L_MFP_PD2_MFP_Pos)

PD2 Pin Function - LCD SEG 4

Definition at line 421 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_GPD3

#define SYS_PD_L_MFP_PD3_MFP_GPD3 (0UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - GPIOD[3]

Definition at line 417 of file sys.h.

## ◆ SYS_PD_L_MFP_PD3_MFP_LCD_S3

#define SYS_PD_L_MFP_PD3_MFP_LCD_S3 (8UL<<SYS_PD_L_MFP_PD3_MFP_Pos)

PD3 Pin Function - LCD SEG 3

Definition at line 418 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_GPD4

#define SYS_PD_L_MFP_PD4_MFP_GPD4 (0UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - GPIOD[4]

Definition at line 413 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_LCD_S2

#define SYS_PD_L_MFP_PD4_MFP_LCD_S2 (8UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - LCD SEG 4

Definition at line 415 of file sys.h.

## ◆ SYS_PD_L_MFP_PD4_MFP_SC1_RST

#define SYS_PD_L_MFP_PD4_MFP_SC1_RST (4UL<<SYS_PD_L_MFP_PD4_MFP_Pos)

PD4 Pin Function - SmartCard1 RST pin

Definition at line 414 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_GPD5

#define SYS_PD_L_MFP_PD5_MFP_GPD5 (0UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - GPIOD[5]

Definition at line 409 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_LCD_COM5

#define SYS_PD_L_MFP_PD5_MFP_LCD_COM5 (8UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - LCD COM 5

Definition at line 411 of file sys.h.

## ◆ SYS_PD_L_MFP_PD5_MFP_LCD_S1

#define SYS_PD_L_MFP_PD5_MFP_LCD_S1 (8UL<<SYS_PD_L_MFP_PD5_MFP_Pos)

PD5 Pin Function - LCD SEG 1

Definition at line 410 of file sys.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_GPD6

#define SYS_PD_L_MFP_PD6_MFP_GPD6 (0UL<<SYS_PD_L_MFP_PD6_MFP_Pos)

PD6 Pin Function - GPIOD[6]

Definition at line 405 of file sys.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_LCD_COM4

#define SYS_PD_L_MFP_PD6_MFP_LCD_COM4 (8UL<<SYS_PD_L_MFP_PD6_MFP_Pos)

PD6 Pin Function - LCD COM 4

Definition at line 407 of file sys.h.

## ◆ SYS_PD_L_MFP_PD6_MFP_LCD_S0

#define SYS_PD_L_MFP_PD6_MFP_LCD_S0 (8UL<<SYS_PD_L_MFP_PD6_MFP_Pos)

PD6 Pin Function - LCD SEG 0

Definition at line 406 of file sys.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_GPD7

#define SYS_PD_L_MFP_PD7_MFP_GPD7 (0UL<<SYS_PD_L_MFP_PD7_MFP_Pos)

PD7 Pin Function - GPIOD[7]

Definition at line 401 of file sys.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_LCD_COM3

#define SYS_PD_L_MFP_PD7_MFP_LCD_COM3 (8UL<<SYS_PD_L_MFP_PD7_MFP_Pos)

PD7 Pin Function - LCD COM 3

Definition at line 403 of file sys.h.

## ◆ SYS_PD_L_MFP_PD7_MFP_SC1_CLK

#define SYS_PD_L_MFP_PD7_MFP_SC1_CLK (4UL<<SYS_PD_L_MFP_PD7_MFP_Pos)

PD7 Pin Function - SmartCard1 clock

Definition at line 402 of file sys.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_GPE8

#define SYS_PE_H_MFP_PE8_MFP_GPE8 (0UL<<SYS_PE_H_MFP_PE8_MFP_Pos)

PE8 Pin Function - GPIOA[8]

Definition at line 497 of file sys.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_LCD_S30

#define SYS_PE_H_MFP_PE8_MFP_LCD_S30 (8UL<<SYS_PE_H_MFP_PE8_MFP_Pos)

PE8 Pin Function - LCD SEG 30

Definition at line 499 of file sys.h.

## ◆ SYS_PE_H_MFP_PE8_MFP_PWM0_CH2

#define SYS_PE_H_MFP_PE8_MFP_PWM0_CH2 (3UL<<SYS_PE_H_MFP_PE8_MFP_Pos)

PE8 Pin Function - PWM0 Channel3 output

Definition at line 498 of file sys.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_GPE9

#define SYS_PE_H_MFP_PE9_MFP_GPE9 (0UL<<SYS_PE_H_MFP_PE9_MFP_Pos)

PE9 Pin Function - GPIOE[9]

Definition at line 493 of file sys.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_LCD_S29

#define SYS_PE_H_MFP_PE9_MFP_LCD_S29 (8UL<<SYS_PE_H_MFP_PE9_MFP_Pos)

PE9 Pin Function - LCD SEG 29

Definition at line 495 of file sys.h.

## ◆ SYS_PE_H_MFP_PE9_MFP_PWM0_CH3

#define SYS_PE_H_MFP_PE9_MFP_PWM0_CH3 (3UL<<SYS_PE_H_MFP_PE9_MFP_Pos)

PE9 Pin Function - PWM0 Channel3 output

Definition at line 494 of file sys.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_GPE0

#define SYS_PE_L_MFP_PE0_MFP_GPE0 (0UL<<SYS_PE_L_MFP_PE0_MFP_Pos)

PE0 Pin Function - GPIOE[0]

Definition at line 489 of file sys.h.

## ◆ SYS_PE_L_MFP_PE0_MFP_SPI0_MOSI0

#define SYS_PE_L_MFP_PE0_MFP_SPI0_MOSI0 (6UL<<SYS_PE_L_MFP_PE0_MFP_Pos)

PE0 Pin Function - SPI0 MOSI[0]

Definition at line 490 of file sys.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_GPE1

#define SYS_PE_L_MFP_PE1_MFP_GPE1 (0UL<<SYS_PE_L_MFP_PE1_MFP_Pos)

PE1 Pin Function - GPIOE[1]

Definition at line 486 of file sys.h.

## ◆ SYS_PE_L_MFP_PE1_MFP_SPI0_MISO0

#define SYS_PE_L_MFP_PE1_MFP_SPI0_MISO0 (6UL<<SYS_PE_L_MFP_PE1_MFP_Pos)

PE1 Pin Function - SPI0 MISO[0]

Definition at line 487 of file sys.h.

## ◆ SYS_PE_L_MFP_PE2_MFP_GPE2

#define SYS_PE_L_MFP_PE2_MFP_GPE2 (0UL<<SYS_PE_L_MFP_PE2_MFP_Pos)

PE2 Pin Function - GPIOE[2]

Definition at line 483 of file sys.h.

## ◆ SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK

#define SYS_PE_L_MFP_PE2_MFP_SPI0_SCLK (6UL<<SYS_PE_L_MFP_PE2_MFP_Pos)

PE2 Pin Function - SPI0 SCLK

Definition at line 484 of file sys.h.

## ◆ SYS_PE_L_MFP_PE3_MFP_GPE3

#define SYS_PE_L_MFP_PE3_MFP_GPE3 (0UL<<SYS_PE_L_MFP_PE3_MFP_Pos)

PE3 Pin Function - GPIOE[3]

Definition at line 480 of file sys.h.

## ◆ SYS_PE_L_MFP_PE3_MFP_SPI0_SS0

#define SYS_PE_L_MFP_PE3_MFP_SPI0_SS0 (6UL<<SYS_PE_L_MFP_PE3_MFP_Pos)

PE3 Pin Function - SPI0 1st slave select pin

Definition at line 481 of file sys.h.

## ◆ SYS_PE_L_MFP_PE4_MFP_GPE4

#define SYS_PE_L_MFP_PE4_MFP_GPE4 (0UL<<SYS_PE_L_MFP_PE4_MFP_Pos)

PE4 Pin Function - GPIOE[4]

Definition at line 477 of file sys.h.

## ◆ SYS_PE_L_MFP_PE4_MFP_SC1_RST

#define SYS_PE_L_MFP_PE4_MFP_SC1_RST (4UL<<SYS_PE_L_MFP_PE4_MFP_Pos)

PE4 Pin Function - SmartCard1 RST

Definition at line 478 of file sys.h.

## ◆ SYS_PE_L_MFP_PE5_MFP_GPE5

#define SYS_PE_L_MFP_PE5_MFP_GPE5 (0UL<<SYS_PE_L_MFP_PE5_MFP_Pos)

PE5 Pin Function - GPIOE[5]

Definition at line 474 of file sys.h.

## ◆ SYS_PE_L_MFP_PE5_MFP_SC1_PWR

#define SYS_PE_L_MFP_PE5_MFP_SC1_PWR (4UL<<SYS_PE_L_MFP_PE5_MFP_Pos)

PE5 Pin Function - SmartCard1 power

Definition at line 475 of file sys.h.

## ◆ SYS_PE_L_MFP_PE6_MFP_GPE6

#define SYS_PE_L_MFP_PE6_MFP_GPE6 (0UL<<SYS_PE_L_MFP_PE6_MFP_Pos)

PE6 Pin Function - GPIOE[6]

Definition at line 471 of file sys.h.

## ◆ SYS_PE_L_MFP_PE6_MFP_SC1_CLK

#define SYS_PE_L_MFP_PE6_MFP_SC1_CLK (4UL<<SYS_PE_L_MFP_PE6_MFP_Pos)

PE6 Pin Function - SmartCard1 clock

Definition at line 472 of file sys.h.

## ◆ SYS_PE_L_MFP_PE7_MFP_GPE7

#define SYS_PE_L_MFP_PE7_MFP_GPE7 (0UL<<SYS_PE_L_MFP_PE7_MFP_Pos)

PE7 Pin Function - GPIOE[7]

Definition at line 468 of file sys.h.

## ◆ SYS_PE_L_MFP_PE7_MFP_SC1_DAT

#define SYS_PE_L_MFP_PE7_MFP_SC1_DAT (4UL<<SYS_PE_L_MFP_PE7_MFP_Pos)

PE7 Pin Function - SmartCard1 data

Definition at line 469 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_GPF0

#define SYS_PF_L_MFP_PF0_MFP_GPF0 (0UL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - GPIOF[0]

Definition at line 532 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_TMR3_CNT

#define SYS_PF_L_MFP_PF0_MFP_TMR3_CNT (2UL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - Timer3 external counter input

Definition at line 533 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_TMR3_OUT

#define SYS_PF_L_MFP_PF0_MFP_TMR3_OUT (0xAUL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - Timer3 toggle out Enable LCD for 100 Pin Package

Definition at line 535 of file sys.h.

## ◆ SYS_PF_L_MFP_PF0_MFP_X32_IN

#define SYS_PF_L_MFP_PF0_MFP_X32_IN (0xFUL<<SYS_PF_L_MFP_PF0_MFP_Pos)

PF0 Pin Function - X32 IN

Definition at line 534 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_GPF1

#define SYS_PF_L_MFP_PF1_MFP_GPF1 (0UL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - GPIOF[1]

Definition at line 527 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_TMR2_CNT

#define SYS_PF_L_MFP_PF1_MFP_TMR2_CNT (2UL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - Timer2 external counter input

Definition at line 528 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_TMR2_OUT

#define SYS_PF_L_MFP_PF1_MFP_TMR2_OUT (0xAUL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - Timer2 toggle out

Definition at line 530 of file sys.h.

## ◆ SYS_PF_L_MFP_PF1_MFP_X32_OUT

#define SYS_PF_L_MFP_PF1_MFP_X32_OUT (0xFUL<<SYS_PF_L_MFP_PF1_MFP_Pos)

PF1 Pin Function - X32 OUT

Definition at line 529 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_EINT1

#define SYS_PF_L_MFP_PF2_MFP_EINT1 (1UL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - External interrupt1 input pin

Definition at line 522 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_GPF2

#define SYS_PF_L_MFP_PF2_MFP_GPF2 (0UL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - GPIOF[2]

Definition at line 521 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_TMR3_CAP

#define SYS_PF_L_MFP_PF2_MFP_TMR3_CAP (2UL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - Timer3 capture input

Definition at line 523 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_UART1_RX

#define SYS_PF_L_MFP_PF2_MFP_UART1_RX (7UL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - UART1 RX

Definition at line 524 of file sys.h.

## ◆ SYS_PF_L_MFP_PF2_MFP_XT1_IN

#define SYS_PF_L_MFP_PF2_MFP_XT1_IN (0xFUL<<SYS_PF_L_MFP_PF2_MFP_Pos)

PF2 Pin Function - XT1 IN

Definition at line 525 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_EINT0

#define SYS_PF_L_MFP_PF3_MFP_EINT0 (1UL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - External interrupt0 input pin

Definition at line 516 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_GPF3

#define SYS_PF_L_MFP_PF3_MFP_GPF3 (0UL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - GPIOF[3]

Definition at line 515 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_TMR2_CAP

#define SYS_PF_L_MFP_PF3_MFP_TMR2_CAP (2UL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - Timer2 capture input

Definition at line 517 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_UART1_TX

#define SYS_PF_L_MFP_PF3_MFP_UART1_TX (7UL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - UART1 TX

Definition at line 518 of file sys.h.

## ◆ SYS_PF_L_MFP_PF3_MFP_XT1_OUT

#define SYS_PF_L_MFP_PF3_MFP_XT1_OUT (0xFUL<<SYS_PF_L_MFP_PF3_MFP_Pos)

PF3 Pin Function - XT1 OUT

Definition at line 519 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_CKO1

#define SYS_PF_L_MFP_PF4_MFP_CKO1 (1UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - Frequency Divider1 output pin

Definition at line 509 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_CLK_Hz

#define SYS_PF_L_MFP_PF4_MFP_CLK_Hz (9UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - 1Hz clock output

Definition at line 512 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_GPF4

#define SYS_PF_L_MFP_PF4_MFP_GPF4 (0UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - GPIOF[4]

Definition at line 508 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_ICE_CLK

#define SYS_PF_L_MFP_PF4_MFP_ICE_CLK (0xFUL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - ICE CLK

Definition at line 513 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_PWM0_CH2

#define SYS_PF_L_MFP_PF4_MFP_PWM0_CH2 (3UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - PWM0 Channel2 output

Definition at line 511 of file sys.h.

## ◆ SYS_PF_L_MFP_PF4_MFP_TMR1_CAP

#define SYS_PF_L_MFP_PF4_MFP_TMR1_CAP (2UL<<SYS_PF_L_MFP_PF4_MFP_Pos)

PF4 Pin Function - Timer1 capture input

Definition at line 510 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_ACMP_C

#define SYS_PF_L_MFP_PF5_MFP_ACMP_C (9UL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - Comparator0 charge/discharge path

Definition at line 505 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_GPF5

#define SYS_PF_L_MFP_PF5_MFP_GPF5 (0UL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - GPIOF[5]

Definition at line 502 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_ICE_DAT

#define SYS_PF_L_MFP_PF5_MFP_ICE_DAT (0xFUL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - ICE DAT

Definition at line 506 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_PWM0_CH3

#define SYS_PF_L_MFP_PF5_MFP_PWM0_CH3 (3UL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - PWM0 Channel3 output

Definition at line 504 of file sys.h.

## ◆ SYS_PF_L_MFP_PF5_MFP_TMR0_CAP

#define SYS_PF_L_MFP_PF5_MFP_TMR0_CAP (2UL<<SYS_PF_L_MFP_PF5_MFP_Pos)

PF5 Pin Function - Timer0 capture input

Definition at line 503 of file sys.h.

## ◆ SYS_VREFCTL_BGP_EN

#define SYS_VREFCTL_BGP_EN ((uint32_t)0x00000001)

Band-gap Enable

Definition at line 61 of file sys.h.

## ◆ SYS_VREFCTL_EXTMODE

#define SYS_VREFCTL_EXTMODE ((uint32_t)0x00000010)

Regulator External Mode

Definition at line 66 of file sys.h.

## ◆ SYS_VREFCTL_REG_EN

#define SYS_VREFCTL_REG_EN ((uint32_t)0x00000002)

Regulator Enable

Definition at line 62 of file sys.h.

## ◆ SYS_VREFCTL_SEL15

#define SYS_VREFCTL_SEL15 ((uint32_t)0x00000000)

Regulator Output Voltage 1.5V

Definition at line 65 of file sys.h.

## ◆ SYS_VREFCTL_SEL18

#define SYS_VREFCTL_SEL18 ((uint32_t)0x00000004)

Regulator Output Voltage 1.8V

Definition at line 64 of file sys.h.

## ◆ SYS_VREFCTL_SEL25

#define SYS_VREFCTL_SEL25 ((uint32_t)0x00000008)

Regulator Output Voltage 2.5V

Definition at line 63 of file sys.h.

## ◆ TMR0_RST

#define TMR0_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR0_RST_Pos )

Timer0 reset is one of the SYS_ResetModule parameter

Definition at line 53 of file sys.h.

## ◆ TMR1_RST

#define TMR1_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR1_RST_Pos )

Timer1 reset is one of the SYS_ResetModule parameter

Definition at line 52 of file sys.h.

## ◆ TMR2_RST

#define TMR2_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR2_RST_Pos )

Timer2 reset is one of the SYS_ResetModule parameter

Definition at line 51 of file sys.h.

## ◆ TMR3_RST

#define TMR3_RST ((0x4<<24) | SYS_IPRST_CTL2_TMR3_RST_Pos )

Timer3 reset is one of the SYS_ResetModule parameter

Definition at line 50 of file sys.h.

## ◆ UART0_RST

#define UART0_RST ((0x4<<24) | SYS_IPRST_CTL2_UART0_RST_Pos )

UART0 reset is one of the SYS_ResetModule parameter

Definition at line 45 of file sys.h.

## ◆ UART1_RST

#define UART1_RST ((0x4<<24) | SYS_IPRST_CTL2_UART1_RST_Pos )

UART1 reset is one of the SYS_ResetModule parameter

Definition at line 44 of file sys.h.