| Nano102_112 Series BSP V3.03.002 The Board Support Package for Nano102_112 Series

Functions
lcd.c File Reference

Nano 102/112 series LCD driver source file. More...

`#include <stdio.h>`
`#include <string.h>`
`#include <stdlib.h>`
`#include "Nano1X2Series.h"`
`#include "lcd.h"`

Go to the source code of this file.

## Functions
void | LCD_SetPixel (uint32_t u32Com, uint32_t u32Seg, uint32_t u32OnFlag)
| Enables a segment on the LCD display. More...
void | LCD_SetAllPixels (uint32_t u32OnOff)
| LCD Enable/Disable all segments. More...
uint32_t | LCD_EnableFrameCounter (uint32_t u32Count)
| Set Frame Count and Enable frame count. More...
void | LCD_DisableFrameCounter (void)
| Disable frame count function. More...
uint32_t | LCD_Open (uint32_t u32DrivingType, uint32_t u32ComNum, uint32_t u32BiasLevel, uint32_t u32FramerateDiv, uint32_t u32DrivingVol)
| LCD Initialization routine. More...
void | LCD_Close (void)
| The function is used to disable LCD controller. More...
uint32_t | LCD_EnableBlink (uint32_t u32ms)
| Enable Blink function in LCD controller. More...
void | LCD_DisableBlink (void)
| Disable Blink function in LCD controller. More...
void | LCD_EnableInt (uint32_t IntSrc)
| This function is used to enable LCD interrupt. More...
void | LCD_DisableInt (uint32_t IntSrc)
| This function is used to disable LCD specified interrupt. More...

## Detailed Description

Nano 102/112 series LCD driver source file.

Version
  V1.00

Revision
  14

Date
  15/06/25 11:37a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013~2014 Nuvoton Technology Corp. All rights reserved.

Definition in file lcd.c.