| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - i -

- Id : STR_CANMSG_T
- IdType : STR_CANMSG_T
- IEN : I2S_T
- IF : CAN_T
- iface_alternate : usb_device
- ifnum : usbhid_dev
- IIDR : CAN_T
- in_streaming : uac_dev_t
- inbuf : usbhid_dev
- INIT : RTC_T
- INT : CAP_T
- INTCTL : PWM_T
- INTEN : CRPT_T, EMAC_T, GPIO_T, OTG_T, PDMA_T, PWM_T, RTC_T, SC_T, SDH_T, UART_T
- interval : urb_t
- INTSRC : EADC_T, GPIO_T
- INTSTS : CRPT_T, EMAC_T, OTG_T, PDMA_T, PS2_T, PWM_T, RTC_T, SC_T, SDH_T, TIMER_T, UART_T
- INTTYPE : GPIO_T
- IPND1 : CAN_T
- IPND2 : CAN_T
- IPRST0 : SYS_T
- IPRST1 : SYS_T
- IPRST2 : SYS_T
- IRCTCTL : SYS_T
- IRCTIEN : SYS_T
- IRCTISTS : SYS_T
- IRDA : UART_T
- IsCardInsert : SD_info_t
- iso_frame_desc : urb_t
- iso_inbuf : uac_dev_t
- iso_outbuf : uac_dev_t
- ISPADDR : FMC_T
- ISPCMD : FMC_T
- ISPCTL : FMC_T
- ISPDAT : FMC_T
- ISPSTS : FMC_T
- ISPTRG : FMC_T