| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
QEI_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CNT
__IO uint32_t | CNTHOLD
__IO uint32_t | CNTLATCH
__IO uint32_t | CNTCMP
__IO uint32_t | CNTMAX
__IO uint32_t | CTR
__IO uint32_t | STATUS

## Detailed Description

    @addtogroup QEI Quadrature Encoder Interface(QEI)
    Memory Mapped Structure for QEI Controller

Definition at line 20087 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h