| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Modules | Macros
I2C Exported Constants
NUC472/NUC442 Device Driver » I2C Driver
Collaboration diagram for I2C Exported Constants:

## Modules
| I2C Exported Functions

## Macros
#define | I2C_STA
#define | I2C_STO
#define | I2C_SI
#define | I2C_AA
#define | I2C_GCMODE_ENABLE
#define | I2C_GCMODE_DISABLE

## Detailed Description

## Macro Definition Documentation

## ◆ I2C_AA

#define I2C_AA

I2C ACK bit value

Definition at line 36 of file i2c.h.

## ◆ I2C_GCMODE_DISABLE

#define I2C_GCMODE_DISABLE

Disable I2C GC Mode

Definition at line 39 of file i2c.h.

## ◆ I2C_GCMODE_ENABLE

#define I2C_GCMODE_ENABLE

Enable I2C GC Mode

Definition at line 38 of file i2c.h.

## ◆ I2C_SI

#define I2C_SI

I2C SI bit value

Definition at line 35 of file i2c.h.

## ◆ I2C_STA

#define I2C_STA

I2C START bit value

Definition at line 33 of file i2c.h.

## ◆ I2C_STO

#define I2C_STO

I2C STOP bit value

Definition at line 34 of file i2c.h.