| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - s -

- SBS : PWM_T
- SCATBA : PDMA_T
- SCATSTS : PDMA_T
- sector_number : mass_disk_t
- sector_size : mass_disk_t
- sectorSize : disk_data_t
- SEED : CRC_T
- SEPIA : CAP_T
- serial : disk_data_t
- SETUP1_0 : USBD_T
- SETUP3_2 : USBD_T
- SETUP5_4 : USBD_T
- SETUP7_6 : USBD_T
- setup_packet : urb_t
- SHA_CTL : CRPT_T
- SHA_DATIN : CRPT_T
- SHA_DGST0 : CRPT_T
- SHA_DGST1 : CRPT_T
- SHA_DGST2 : CRPT_T
- SHA_DGST3 : CRPT_T
- SHA_DGST4 : CRPT_T
- SHA_DGST5 : CRPT_T
- SHA_DGST6 : CRPT_T
- SHA_DGST7 : CRPT_T
- SHA_DMACNT : CRPT_T
- SHA_KEYCNT : CRPT_T
- SHA_SADDR : CRPT_T
- SHA_STS : CRPT_T
- SIMUSEL : EADC_T
- SLEWCTL : GPIO_T
- slow : usb_device
- SMTEN : GPIO_T
- speed : usb_device
- SPR : RTC_T
- SPRCTL : RTC_T
- SRAM0_ERRADDR : SYS_T
- SRAM1_ERRADDR : SYS_T
- SRAM_INTCTL : SYS_T
- SRAM_STATUS : SYS_T
- SSCTL : SPI_T
- start_frame : urb_t
- STATUS : ACMP_T, CAN_T, CLK_T, ECAP_T, EPWM_T, I2C_T, I2S_T
- status : iso_pkt_t
- STATUS : OPA_T, OTG_T, PS2_T, QEI_T, SC_T, SPI_T
- status : urb_t
- STATUS : WWDT_T
- STATUS0 : ADC_T, EADC_T
- STATUS1 : ADC_T, EADC_T
- STOP : PDMA_T
- STRIDE : CAP_T
- string_langid : usb_device
- SWREQ : PDMA_T
- SWTRG : EADC_T