| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
I2C_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | ADDR0
__IO uint32_t | DAT
__I uint32_t | STATUS
__IO uint32_t | CLKDIV
__IO uint32_t | TOCTL
__IO uint32_t | ADDR1
__IO uint32_t | ADDR2
__IO uint32_t | ADDR3
__IO uint32_t | ADDRMSK0
__IO uint32_t | ADDRMSK1
__IO uint32_t | ADDRMSK2
__IO uint32_t | ADDRMSK3
__IO uint32_t | WKCTL
__IO uint32_t | WKSTS

## Detailed Description

    @addtogroup I2C Inter-IC Bus Controller(I2C)
    Memory Mapped Structure for I2C Controller

Definition at line 16820 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h