| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Modules | Variables
CAP Driver
NUC472/NUC442 Device Driver
Collaboration diagram for CAP Driver:

## Modules
| CAP Exported Constants

## Variables
int32_t | g_CAP_i32ErrCode = 0

## Detailed Description

## Variable Documentation

## ◆ g_CAP_i32ErrCode

int32_t g_CAP_i32ErrCode = 0

CAP global error code

Definition at line 22 of file cap.c.