| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions
uac_driver.c File Reference

NUC472/NUC442 MCU USB Host Audio Class driver. More...

`#include <stdio.h>`
`#include <string.h>`
`#include "NUC472_442.h"`
`#include "usbh_core.h"`
`#include "usbh_uac.h"`
`#include "uac.h"`
Include dependency graph for uac_driver.c:

Go to the source code of this file.

## Functions
void | UAC_Init (void)
| Initialize this USB Audio Class driver. More...
UAC_DEV_T * | UAC_GetDeviceList (void)
| Get a list of currently connected USB Audio Class devices. More...

## Detailed Description

NUC472/NUC442 MCU USB Host Audio Class driver.

Version
  V1.00

Revision
  1

Date
  14/10/31 10:32a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Version
  V1.00

Revision
  1

Date
  14/10/31 10:32a

Note
  Support mono and stero audio input and output. SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file uac_driver.c.