| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
STR_CANMSG_T Struct Reference
NUC472/NUC442 Device Driver » CAN Driver » CAN Exported Type Defines

`#include <can.h>`

## Data Fields
uint32_t | IdType
uint32_t | FrameType
uint32_t | Id
uint8_t | DLC
uint8_t | Data [8]

## Detailed Description

CAN message structure.

Definition at line 53 of file can.h.

The documentation for this struct was generated from the following file:

- StdDriver/inc/can.h