| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Fields
EPWM_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | STATUS
__IO uint32_t | PERIOD
__IO uint32_t | CMPDAT [3]
__IO uint32_t | MSKEN
__IO uint32_t | MSK
__IO uint32_t | ASYMCMP0
__IO uint32_t | ASYMCMP2
__IO uint32_t | ASYMCMP4
__IO uint32_t | DTCTL
__IO uint32_t | BRKOUT
__IO uint32_t | NPCTL
__IO uint32_t | ASYMCTL
__IO uint32_t | PERIODCNT
__IO uint32_t | EINTCTL
__IO uint32_t | OUTEN0

## Detailed Description

    @addtogroup EPWM Enhanced PWM Generator(EPWM)
    Memory Mapped Structure for EPWM Controller

Definition at line 13932 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h