| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions
UmasDriver.c File Reference

NUC472/NUC442 MCU USB Host Mass Storage Library. More...

`#include <stdio.h>`
`#include <string.h>`
`#include "NUC472_442.h"`
`#include "usbh_core.h"`
`#include "Umas.h"`
`#include "diskio.h"`
`#include "usbh_umas.h"`
Include dependency graph for UmasDriver.c:

Go to the source code of this file.

## Functions
int32_t | USBH_MassInit (void)
| Initialize USB Host Mass Storage driver. More...
int32_t | USBH_MassGetDiskList (mass_disk_t *dlist[], int max)
| Obtain the list of currently connected USB Mass Storage disk. More...

## Detailed Description

NUC472/NUC442 MCU USB Host Mass Storage Library.

Version
  V1.00

Revision
  6

Date
  15/03/23 8:34a

Note
  Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file UmasDriver.c.