| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Data Structures | Functions
usbh_umas.h File Reference

USB Host Mass Storage driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | mass_disk_t

## Functions
int32_t | USBH_MassInit (void)
| Initialize USB Host Mass Storage driver. More...
int32_t | USBH_MassGetDiskList (mass_disk_t *dlist[], int max)
| Obtain the list of currently connected USB Mass Storage disk. More...
int32_t | USBH_MassRawRead (mass_disk_t *disk, uint32_t sectorN, int32_t scnt, uint8_t *buff)
| Read raw data from connected USB Mass Storage disk. More...
int32_t | USBH_MassRawWrite (mass_disk_t *disk, uint32_t sectorN, int32_t scnt, uint8_t *buff)
| Write raw data to connected USB Mass Storage disk. More...

## Detailed Description

USB Host Mass Storage driver header file.

Version
  V1.00 $Revision 2 $

Date
  14/10/31 10:31a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file usbh_umas.h.