| NUC472_NUC442_BSP V3.03.003 The Board Support Package for NUC472/NUC442

Functions
eadc.c File Reference

NUC472/NUC442 EADC driver source file. More...

`#include "NUC472_442.h"`
Include dependency graph for eadc.c:

Go to the source code of this file.

## Functions
void | EADC_Open (EADC_T *eadc, uint32_t u32InputMode)
| This function make EADC_module be ready to convert. More...
void | EADC_Close (EADC_T *eadc)
| Disable EADC_module. More...
void | EADC_ConfigSampleModule (EADC_T *eadc, uint32_t u32ModuleNum, uint32_t u32TriggerSrc, uint32_t u32Channel)
| Configure the sample control logic module. More...
void | EADC_SetTriggerDelayTime (EADC_T *eadc, uint32_t u32ModuleNum, uint32_t u32TriggerDelayTime, uint32_t u32DelayClockDivider)
| Set trigger delay time. More...
void | EADC_SetExtendSampleTime (EADC_T *eadc, uint32_t u32ModuleNum, uint32_t u32ExtendSampleTime)
| Set EADC extend sample time. More...

## Detailed Description

NUC472/NUC442 EADC driver source file.

Version
  V1.00

Revision
  7

Date
  15/12/01 10:12a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2015 Nuvoton Technology Corp. All rights reserved.

Definition in file eadc.c.